/***********************************************************************
 Physical Constraint file 
 Version:1.8.0Alpha
 Created Time:   Tue Jan 30 18:00:21 2018
 Device:         GW2AR-18
 Package:        LQFP176
************************************************************************/
IO_LOC "clk" 32;
IO_LOC "display" 148;
IO_LOC "sr_in" 143;
IO_LOC "init_calib_complete" 162;
IO_LOC "pll_out" 149;
IO_LOC "rst_n" 96;
IO_LOC "seg_en[0]" 30;
IO_LOC "seg_en[1]" 28;
IO_LOC "seg_en[2]" 26;
IO_LOC "seg_en[3]" 24;
IO_LOC "show_data[0]" 53;
IO_LOC "show_data[1]" 51;
IO_LOC "show_data[2]" 49;
IO_LOC "show_data[3]" 47;
IO_LOC "sw" 146;
IO_LOC "test_out[1]" 139;
IO_LOC "test_out[2]" 135;
IO_LOC "test_out[3]" 141;
IO_LOC "test_out[4]" 142;
IO_LOC "test_out[5]" 144;
IO_LOC "test_out[0]" 138;
IO_PORT "seg_en[3]"  IO_TYPE=LVCMOS25 SINGLE_RESISTOR=OFF BANK_VCCIO=2.5;
IO_PORT "show_data[0]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "show_data[1]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "show_data[2]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "show_data[3]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "pll_out"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "test_out[1]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "test_out[2]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "test_out[3]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "test_out[4]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "test_out[5]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "sr_in"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "test_out[0]"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "clk"  IO_TYPE=LVCMOS25 SINGLE_RESISTOR=OFF BANK_VCCIO=2.5;
IO_PORT "rst_n"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "display"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "sw"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "read_in"  IO_TYPE=LVCMOS25;
IO_PORT "init_calib_complete"  IO_TYPE=LVCMOS25 BANK_VCCIO=2.5;
IO_PORT "seg_en[0]"  IO_TYPE=LVCMOS25 SINGLE_RESISTOR=OFF BANK_VCCIO=2.5;
IO_PORT "seg_en[1]"  IO_TYPE=LVCMOS25 SINGLE_RESISTOR=OFF BANK_VCCIO=2.5;
IO_PORT "seg_en[2]"  IO_TYPE=LVCMOS25 SINGLE_RESISTOR=OFF BANK_VCCIO=2.5;
