Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH256K_REG_IF\project\impl\synthesize\rev_1\FLASH256K_REG_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH256K_REG_IF\project\src\FLASH256K_REG_IF.cst
Timing Constraints File | ---
GOWIN Version | V1.9.2.01Beta
Part Number | GW1N-LV4LQ144C6/I5
Created Time | Tue Oct 22 17:09:15 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 23.607
Quiescent Power (mW) | 4.491
Dynamic Power (mW) | 19.116

## Thermal Information:

Junction Temperature | 25.234
Theta JA | 10.100
Max Allowed Ambient Temperature | 84.762

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 14.108 | 2.523 | 19.957
VCCX | 2.500 | 0.509 | 0.341 | 2.125
VCCO18 | 1.800 | 0.508 | 0.340 | 1.526

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 4.290 | NA | 12.500
IO | 4.670 | 1.872 | 14.931

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
tb | 16.291 | 4.290(4.166) | 12.001(11.268)
tb/u_gowin_flash_controller_top/ | 15.435 | 4.166(4.166) | 11.268(11.268)
tb/u_gowin_flash_controller_top/u_Flash_Ctroller_256K/ | 15.435 | 4.166(3.645) | 11.268(8.327)
tb/u_gowin_flash_controller_top/u_Flash_Ctroller_256K/u_ER_UFM/ | 4.821 | 1.786(0.000) | 3.035(0.000)
tb/u_gowin_flash_controller_top/u_Flash_Ctroller_256K/u_GW_USER_FLASH_256K/ | 1.890 | 0.219(0.000) | 1.671(0.000)
tb/u_gowin_flash_controller_top/u_Flash_Ctroller_256K/u_RD_UFM/ | 0.558 | 0.101(0.000) | 0.457(0.000)
tb/u_gowin_flash_controller_top/u_Flash_Ctroller_256K/u_WR_UFM/ | 4.703 | 1.539(0.000) | 3.164(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
DEFAULT_CLK | 100.000 | 16.318