Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH608K_WB_IF\project\impl\synthesize\rev_1\FLASH608K_WB_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH608K_WB_IF\project\src\FLASH608K_WB_IF.cst
Timing Constraints File | ---
GOWIN Version | V1.9.2.01Beta
Part Number | GW1N-LV9LQ144C6/I5
Created Time | Tue Oct 22 17:14:42 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 28.850
Quiescent Power (mW) | 4.492
Dynamic Power (mW) | 24.358

## Thermal Information:

Junction Temperature | 25.287
Theta JA | 10.100
Max Allowed Ambient Temperature | 84.709

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 18.476 | 2.524 | 25.200
VCCX | 2.500 | 0.509 | 0.341 | 2.125
VCCO18 | 1.800 | 0.508 | 0.340 | 1.526

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 4.753 | NA | 12.500
IO | 4.670 | 1.872 | 14.931

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
tb | 21.531 | 4.753(4.533) | 16.778(15.022)
tb/Gowin_Flash_Controller_template/ | 19.555 | 4.533(4.533) | 15.022(15.022)
tb/Gowin_Flash_Controller_template/u_Wishbone_Master_Top_608K/ | 19.555 | 4.533(4.340) | 15.022(13.030)
tb/Gowin_Flash_Controller_template/u_Wishbone_Master_Top_608K/u_Flash_Ctroller_608K/ | 17.370 | 4.340(3.659) | 13.030(9.136)
tb/Gowin_Flash_Controller_template/u_Wishbone_Master_Top_608K/u_Flash_Ctroller_608K/u_ER_UFM/ | 4.613 | 1.686(0.000) | 2.926(0.000)
tb/Gowin_Flash_Controller_template/u_Wishbone_Master_Top_608K/u_Flash_Ctroller_608K/u_GW_USER_FLASH_608K/ | 2.245 | 0.224(0.000) | 2.020(0.000)
tb/Gowin_Flash_Controller_template/u_Wishbone_Master_Top_608K/u_Flash_Ctroller_608K/u_RD_UFM/ | 0.655 | 0.069(0.000) | 0.586(0.000)
tb/Gowin_Flash_Controller_template/u_Wishbone_Master_Top_608K/u_Flash_Ctroller_608K/u_WR_UFM/ | 5.283 | 1.679(0.000) | 3.604(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
DEFAULT_CLK | 100.000 | 21.560