Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH96K_REG_IF\project\impl\synthesize\rev_1\FLASH96K_REG_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH96K_REG_IF\project\src\FLASH96K_REF_IF.cst
Timing Constraints File | ---
GOWIN Version | V1.9.2.01Beta
Part Number | GW1N-LV1LQ144C6/I5
Created Time | Tue Oct 22 17:05:34 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 6.917
Quiescent Power (mW) | 6.542
Dynamic Power (mW) | 0.375

## Thermal Information:

Junction Temperature | 25.132
Theta JA | 22.100
Max Allowed Ambient Temperature | 84.847

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 0.250 | 2.660 | 3.492
VCCX | 2.500 | 0.018 | 0.779 | 1.992
VCCO18 | 1.800 | 0.017 | 0.779 | 1.433

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
IO | 4.381 | 4.285 | 0.325
PLL | 0.279 | NA | NA

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
tb | 0.279 | 0.279(0.279) | 0.000(0.000)
tb/u_gowin_flash_controller_top/ | 0.000 | 0.000(0.000) | 0.000(0.000)
tb/u_gowin_flash_controller_top/u_User_Flash_Ctroller_Top_96K/ | 0.000 | 0.000(0.000) | 0.000(0.000)
tb/u_gowin_flash_controller_top/u_User_Flash_Ctroller_Top_96K/u_Flash_ctroller_96K/ | 0.000 | 0.000(0.000) | 0.000(0.000)
tb/u_pll_10M/ | 0.279 | 0.279(0.000) | 0.000(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
NO CLOCK DOMAIN | 0.000 | 0.000
u_pll_10M/pll_inst/CLKIN.default_clk | 50.000 | 0.279