PnR Analysis Report

- PnR Messages
- PnR Details
  - Placer
  - Resource Usage Summary
  - I/O Bank Usage Summary
  - Router
  - Global Clock Usage Summary
  - Global Clock Signals
  - Pinout by Port Name
  - All Package Pins
  - Memory Usage

# PnR Messages

Report Title | Gowin PnR Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH96K_REG_IF\project\impl\synthesize\rev_1\FLASH96K_REG_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH96K_REG_IF\project\src\FLASH96K_REF_IF.cst
Timing Constraints File | ---
GOWIN Version | V1.9.2.01Beta
Part Number | GW1N-LV1LQ144C6/I5
Created Time | Tue Oct 22 17:05:34 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# PnR Details

## Placer:

Starting Placer:

Placement Phase 0 ... REAL time: 0.034 secs

Placement Phase 1 ... REAL time: 0.039 secs

Placement Phase 2 ... REAL time: 0.098 secs

Placement Phase 3 ... REAL time: 0.848 secs

Total REAL time to Placement completion: 1.019 secs.

## Resource Usage Summary:

Resource | Usage | Utilization
Logics | 301/1152 | 26%
--LUTs,ALUs,ROM16s | 301(224 LUTs, 77 ALUs, 0 ROM16s) | -
--SSRAMs(RAM16s) | 0 | -
Registers | 191/1155 | 16%
--logic Registers | 160/864 | 18%
--I/O Registers | 31/291 | 10%
CLSs | 181/576 | 31%
I/O Ports | 79 | -
I/O Bufs | 77 | -
--Input Bufs | 2 | -
--Output Bufs | 75 | -
--Inout Bufs | 0 | -
IOLOGICs | 0 | -
IODELAYs | 0/97 | 0%
BSRAMs | 0/4 | 0%
PLLs | 1/1 | 100%
DCSs | 0/4 | 0%
DQCEs | 0/12 | 0%
OSCs | 0/1 | 0%
User Flashes | 1/1 | 100%
CLKDIVs | 0/2 | 0%
DLLDLYs | 0/2 | 0%
DHCENs | 0/4 | 0%

## I/O Bank Usage Summary:

I/O Bank | Usage
bank 0 | 23/31(74%)
bank 1 | 14/26(53%)
bank 2 | 23/34(67%)
bank 3 | 17/26(65%)

## Router:

Starting Router:

Route Phase 0: 708 unrouted; REAL time: 0 secs

Route Phase 1: 345 unrouted; REAL time: 0.017 secs

Route Phase 2: 0 unrouted; REAL time: 0.063 secs

Total REAL time to Router completion: 0.08 secs.

## Global Clock Usage Summary:

Global Clock | Usage
PRIMARY | 1/8(12%)
SECONDARY | 1/8(12%)
GCLK_PIN | 5/5(100%)
PLL | 1/1(100%)
CLKDIV | 0/2(0%)
DLLDLY | 0/2(0%)

## Global Clock Signals:

Signal | Global Clock | Location
clk_sys_c | PRIMARY | RIGHT
un1_rst_n_dly | SECONDARY | -

## Pinout by Port Name:

Port Name | Loc./Bank | Dir. | Site | I/O Type | Drive | Pull Mode | Slew Rate | Clamp | OpenDrain | VREF | BankVccio
clk_sys | 11/3 | in | IOL5[A] | LVCMOS33 | NA | UP | NA | NA | NA | NA | 1.8
rstn | 41/2 | in | IOB3[B] | LVCMOS18 | NA | UP | NA | NA | NA | NA | 1.8
key | 40/2 | in | IOB3[A] | LVCMOS33 | NA | UP | NA | NA | NA | NA | 1.8
key2 | 39/2 | in | IOB2[B] | LVCMOS18 | NA | UP | NA | NA | NA | NA | 1.8
data_in_flag | 128/0 | out | IOT11[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out_flag | 121/0 | out | IOT13[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[0] | 126/0 | out | IOT11[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[1] | 122/0 | out | IOT13[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[2] | 123/0 | out | IOT12[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[3] | 34/3 | out | IOL10[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[4] | 32/3 | out | IOL10[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[5] | 38/2 | out | IOB2[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[6] | 30/3 | out | IOL9[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[7] | 29/3 | out | IOL9[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[8] | 27/3 | out | IOL8[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[9] | 25/3 | out | IOL7[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[10] | 28/3 | out | IOL8[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[11] | 26/3 | out | IOL7[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[12] | 23/3 | out | IOL6[I] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[13] | 15/3 | out | IOL6[C] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[14] | 12/3 | out | IOL5[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[15] | 10/3 | out | IOL4[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[16] | 9/3 | out | IOL4[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[17] | 7/3 | out | IOL3[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[18] | 6/3 | out | IOL2[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[19] | 4/3 | out | IOL2[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[20] | 3/0 | out | IOT2[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[21] | 140/0 | out | IOT5[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[22] | 142/0 | out | IOT4[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[23] | 139/0 | out | IOT5[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[24] | 137/0 | out | IOT6[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[25] | 138/0 | out | IOT6[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[26] | 135/0 | out | IOT7[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[27] | 133/0 | out | IOT8[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[28] | 134/0 | out | IOT8[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[29] | 132/0 | out | IOT9[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[30] | 129/0 | out | IOT10[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_out[31] | 130/0 | out | IOT10[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
page_address[0] | 51/2 | out | IOB8[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
page_address[1] | 50/2 | out | IOB8[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
page_address[2] | 56/2 | out | IOB10[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
page_address[3] | 46/2 | out | IOB6[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
page_address[4] | 49/2 | out | IOB7[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
page_address[5] | 48/2 | out | IOB7[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[0] | 114/0 | out | IOT17[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[1] | 116/0 | out | IOT16[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[2] | 117/0 | out | IOT15[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[3] | 104/1 | out | IOR2[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[4] | 106/1 | out | IOR2[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[5] | 113/0 | out | IOT17[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[6] | 99/1 | out | IOR4[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[7] | 100/1 | out | IOR4[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[8] | 101/1 | out | IOR3[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[9] | 84/1 | out | IOR7[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[10] | 86/1 | out | IOR6[I] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[11] | 98/1 | out | IOR5[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[12] | 80/1 | out | IOR9[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[13] | 82/1 | out | IOR8[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[14] | 83/1 | out | IOR7[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[15] | 76/1 | out | IOR10[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[16] | 78/1 | out | IOR10[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[17] | 79/1 | out | IOR9[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[18] | 71/2 | out | IOB17[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[19] | 70/2 | out | IOB17[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[20] | 75/2 | out | IOB19[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[21] | 67/2 | out | IOB15[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[22] | 66/2 | out | IOB15[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[23] | 68/2 | out | IOB16[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[24] | 63/2 | out | IOB13[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[25] | 65/2 | out | IOB14[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[26] | 64/2 | out | IOB14[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[27] | 58/2 | out | IOB11[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[28] | 61/2 | out | IOB12[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[29] | 60/2 | out | IOB12[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[30] | 54/2 | out | IOB9[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
data_in[31] | 52/2 | out | IOB9[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
write_en | 57/2 | out | IOB10[B] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
read_en | 118/0 | out | IOT15[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8
wr_cycle | 120/0 | out | IOT14[A] | LVCMOS18 | 8 | UP | FAST | NA | OFF | NA | 1.8

## All Package Pins:

Loc./Bank | Signal | Dir. | Site | Io Type | Pull Mode | Hysteresis | DiffResistor | SingleResistor
3/0 | data_out[20] | out | IOT2[A] | LVCMOS18 | UP | NA | NA | NA | 144/0 | UNUSED | - | IOT2[B] | - | - | - | - | - | 143/0 | UNUSED | - | IOT3[B] | - | - | - | - | - | 142/0 | data_out[22] | out | IOT4[A] | LVCMOS18 | UP | NA | NA | NA | 141/0 | UNUSED | - | IOT4[B] | - | - | - | - | - | 140/0 | data_out[21] | out | IOT5[A] | LVCMOS18 | UP | NA | NA | NA | 139/0 | data_out[23] | out | IOT5[B] | LVCMOS18 | UP | NA | NA | NA | 138/0 | data_out[25] | out | IOT6[A] | LVCMOS18 | UP | NA | NA | NA | 137/0 | data_out[24] | out | IOT6[B] | LVCMOS18 | UP | NA | NA | NA | 136/0 | UNUSED | - | IOT7[A] | - | - | - | - | - | 135/0 | data_out[26] | out | IOT7[B] | LVCMOS18 | UP | NA | NA | NA | 134/0 | data_out[28] | out | IOT8[A] | LVCMOS18 | UP | NA | NA | NA | 133/0 | data_out[27] | out | IOT8[B] | LVCMOS18 | UP | NA | NA | NA | 132/0 | data_out[29] | out | IOT9[A] | LVCMOS18 | UP | NA | NA | NA | 131/0 | UNUSED | - | IOT9[B] | - | - | - | - | - | 130/0 | data_out[31] | out | IOT10[A] | LVCMOS18 | UP | NA | NA | NA | 129/0 | data_out[30] | out | IOT10[B] | LVCMOS18 | UP | NA | NA | NA | 128/0 | data_in_flag | out | IOT11[A] | LVCMOS18 | UP | NA | NA | NA | 126/0 | data_out[0] | out | IOT11[B] | LVCMOS18 | UP | NA | NA | NA | 124/0 | UNUSED | - | IOT12[A] | - | - | - | - | - | 123/0 | data_out[2] | out | IOT12[B] | LVCMOS18 | UP | NA | NA | NA | 122/0 | data_out[1] | out | IOT13[A] | LVCMOS18 | UP | NA | NA | NA | 121/0 | data_out_flag | out | IOT13[B] | LVCMOS18 | UP | NA | NA | NA | 120/0 | wr_cycle | out | IOT14[A] | LVCMOS18 | UP | NA | NA | NA | 119/0 | UNUSED | - | IOT14[B] | - | - | - | - | - | 118/0 | read_en | out | IOT15[A] | LVCMOS18 | UP | NA | NA | NA | 117/0 | data_in[2] | out | IOT15[B] | LVCMOS18 | UP | NA | NA | NA | 116/0 | data_in[1] | out | IOT16[A] | LVCMOS18 | UP | NA | NA | NA | 115/0 | UNUSED | - | IOT16[B] | - | - | - | - | - | 114/0 | data_in[0] | out | IOT17[A] | LVCMOS18 | UP | NA | NA | NA | 113/0 | data_in[5] | out | IOT17[B] | LVCMOS18 | UP | NA | NA | NA | 38/2 | data_out[5] | out | IOB2[A] | LVCMOS18 | UP | NA | NA | NA | 39/2 | key2 | in | IOB2[B] | LVCMOS18 | UP | NONE | NA | NA | 40/2 | key | in | IOB3[A] | LVCMOS33 | UP | NONE | NA | NA | 41/2 | rstn | in | IOB3[B] | LVCMOS18 | UP | NONE | NA | NA | 42/2 | UNUSED | - | IOB4[A] | - | - | - | - | - | 43/2 | UNUSED | - | IOB4[B] | - | - | - | - | - | 44/2 | UNUSED | - | IOB5[A] | - | - | - | - | - | 45/2 | UNUSED | - | IOB5[B] | - | - | - | - | - | 46/2 | page_address[3] | out | IOB6[A] | LVCMOS18 | UP | NA | NA | NA | 47/2 | UNUSED | - | IOB6[B] | - | - | - | - | - | 48/2 | page_address[5] | out | IOB7[A] | LVCMOS18 | UP | NA | NA | NA | 49/2 | page_address[4] | out | IOB7[B] | LVCMOS18 | UP | NA | NA | NA | 50/2 | page_address[1] | out | IOB8[A] | LVCMOS18 | UP | NA | NA | NA | 51/2 | page_address[0] | out | IOB8[B] | LVCMOS18 | UP | NA | NA | NA | 52/2 | data_in[31] | out | IOB9[A] | LVCMOS18 | UP | NA | NA | NA | 54/2 | data_in[30] | out | IOB9[B] | LVCMOS18 | UP | NA | NA | NA | 56/2 | page_address[2] | out | IOB10[A] | LVCMOS18 | UP | NA | NA | NA | 57/2 | write_en | out | IOB10[B] | LVCMOS18 | UP | NA | NA | NA | 58/2 | data_in[27] | out | IOB11[A] | LVCMOS18 | UP | NA | NA | NA | 59/2 | UNUSED | - | IOB11[B] | - | - | - | - | - | 60/2 | data_in[29] | out | IOB12[A] | LVCMOS18 | UP | NA | NA | NA | 61/2 | data_in[28] | out | IOB12[B] | LVCMOS18 | UP | NA | NA | NA | 62/2 | UNUSED | - | IOB13[A] | - | - | - | - | - | 63/2 | data_in[24] | out | IOB13[B] | LVCMOS18 | UP | NA | NA | NA | 64/2 | data_in[26] | out | IOB14[A] | LVCMOS18 | UP | NA | NA | NA | 65/2 | data_in[25] | out | IOB14[B] | LVCMOS18 | UP | NA | NA | NA | 66/2 | data_in[22] | out | IOB15[A] | LVCMOS18 | UP | NA | NA | NA | 67/2 | data_in[21] | out | IOB15[B] | LVCMOS18 | UP | NA | NA | NA | 68/2 | data_in[23] | out | IOB16[A] | LVCMOS18 | UP | NA | NA | NA | 69/2 | UNUSED | - | IOB16[B] | - | - | - | - | - | 70/2 | data_in[19] | out | IOB17[A] | LVCMOS18 | UP | NA | NA | NA | 71/2 | data_in[18] | out | IOB17[B] | LVCMOS18 | UP | NA | NA | NA | 72/2 | UNUSED | - | IOB19[A] | - | - | - | - | - | 75/2 | data_in[20] | out | IOB19[B] | LVCMOS18 | UP | NA | NA | NA | 4/3 | data_out[19] | out | IOL2[A] | LVCMOS18 | UP | NA | NA | NA | 6/3 | data_out[18] | out | IOL2[B] | LVCMOS18 | UP | NA | NA | NA | 7/3 | data_out[17] | out | IOL3[A] | LVCMOS18 | UP | NA | NA | NA | 8/3 | UNUSED | - | IOL3[B] | - | - | - | - | - | 9/3 | data_out[16] | out | IOL4[A] | LVCMOS18 | UP | NA | NA | NA | 10/3 | data_out[15] | out | IOL4[B] | LVCMOS18 | UP | NA | NA | NA | 11/3 | clk_sys | in | IOL5[A] | LVCMOS33 | UP | NONE | NA | OFF | 12/3 | data_out[14] | out | IOL5[B] | LVCMOS18 | UP | NA | NA | NA | 13/3 | UNUSED | - | IOL6[A] | - | - | - | - | - | 14/3 | UNUSED | - | IOL6[B] | - | - | - | - | - | 15/3 | data_out[13] | out | IOL6[C] | LVCMOS18 | UP | NA | NA | NA | 16/3 | UNUSED | - | IOL6[D] | - | - | - | - | - | 18/3 | UNUSED | - | IOL6[E] | - | - | - | - | - | 20/3 | UNUSED | - | IOL6[F] | - | - | - | - | - | 21/3 | UNUSED | - | IOL6[G] | - | - | - | - | - | 22/3 | UNUSED | - | IOL6[H] | - | - | - | - | - | 23/3 | data_out[12] | out | IOL6[I] | LVCMOS18 | UP | NA | NA | NA | 24/3 | UNUSED | - | IOL6[J] | - | - | - | - | - | 25/3 | data_out[9] | out | IOL7[A] | LVCMOS18 | UP | NA | NA | NA | 26/3 | data_out[11] | out | IOL7[B] | LVCMOS18 | UP | NA | NA | NA | 27/3 | data_out[8] | out | IOL8[A] | LVCMOS18 | UP | NA | NA | NA | 28/3 | data_out[10] | out | IOL8[B] | LVCMOS18 | UP | NA | NA | NA | 29/3 | data_out[7] | out | IOL9[A] | LVCMOS18 | UP | NA | NA | NA | 30/3 | data_out[6] | out | IOL9[B] | LVCMOS18 | UP | NA | NA | NA | 32/3 | data_out[4] | out | IOL10[A] | LVCMOS18 | UP | NA | NA | NA | 34/3 | data_out[3] | out | IOL10[B] | LVCMOS18 | UP | NA | NA | NA | 106/1 | data_in[4] | out | IOR2[A] | LVCMOS18 | UP | NA | NA | NA | 104/1 | data_in[3] | out | IOR2[B] | LVCMOS18 | UP | NA | NA | NA | 102/1 | UNUSED | - | IOR3[A] | - | - | - | - | - | 101/1 | data_in[8] | out | IOR3[B] | LVCMOS18 | UP | NA | NA | NA | 100/1 | data_in[7] | out | IOR4[A] | LVCMOS18 | UP | NA | NA | NA | 99/1 | data_in[6] | out | IOR4[B] | LVCMOS18 | UP | NA | NA | NA | 98/1 | data_in[11] | out | IOR5[A] | LVCMOS18 | UP | NA | NA | NA | 97/1 | UNUSED | - | IOR5[B] | - | - | - | - | - | 96/1 | UNUSED | - | IOR6[A] | - | - | - | - | - | 95/1 | UNUSED | - | IOR6[B] | - | - | - | - | - | 94/1 | UNUSED | - | IOR6[C] | - | - | - | - | - | 93/1 | UNUSED | - | IOR6[D] | - | - | - | - | - | 92/1 | UNUSED | - | IOR6[E] | - | - | - | - | - | 90/1 | UNUSED | - | IOR6[F] | - | - | - | - | - | 88/1 | UNUSED | - | IOR6[G] | - | - | - | - | - | 87/1 | UNUSED | - | IOR6[H] | - | - | - | - | - | 86/1 | data_in[10] | out | IOR6[I] | LVCMOS18 | UP | NA | NA | NA | 85/1 | UNUSED | - | IOR6[J] | - | - | - | - | - | 84/1 | data_in[9] | out | IOR7[A] | LVCMOS18 | UP | NA | NA | NA | 83/1 | data_in[14] | out | IOR7[B] | LVCMOS18 | UP | NA | NA | NA | 82/1 | data_in[13] | out | IOR8[A] | LVCMOS18 | UP | NA | NA | NA | 81/1 | UNUSED | - | IOR8[B] | - | - | - | - | - | 80/1 | data_in[12] | out | IOR9[A] | LVCMOS18 | UP | NA | NA | NA | 79/1 | data_in[17] | out | IOR9[B] | LVCMOS18 | UP | NA | NA | NA | 78/1 | data_in[16] | out | IOR10[A] | LVCMOS18 | UP | NA | NA | NA | 76/1 | data_in[15] | out | IOR10[B] | LVCMOS18 | UP | NA | NA | NA

Placement and routing completed.

Memory usage: 83MB.