Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH256K_WB_IF\project\impl\synthesize\rev_1\FLASH256K_WB_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH256K_WB_IF\project\src\FLASH256K_WB_IF.cst
Timing Constraints File | ---
GOWIN Version | V1.9.2.01Beta
Part Number | GW1N-LV4LQ144C6/I5
Created Time | Tue Oct 22 17:11:30 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 27.479
Quiescent Power (mW) | 4.492
Dynamic Power (mW) | 22.987

## Thermal Information:

Junction Temperature | 25.273
Theta JA | 10.100
Max Allowed Ambient Temperature | 84.722

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 17.333 | 2.524 | 23.828
VCCX | 2.500 | 0.509 | 0.341 | 2.125
VCCO18 | 1.800 | 0.508 | 0.340 | 1.526

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 4.727 | NA | 12.500
IO | 4.670 | 1.872 | 14.931

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
tb | 20.160 | 4.727(4.502) | 15.433(13.703)
tb/flash_controller_inst/ | 18.205 | 4.502(4.502) | 13.703(13.703)
tb/flash_controller_inst/u_Wishbone_Master_Top_256K/ | 18.205 | 4.502(4.285) | 13.703(11.605)
tb/flash_controller_inst/u_Wishbone_Master_Top_256K/u_Flash_Ctroller_256K/ | 15.890 | 4.285(3.651) | 11.605(8.090)
tb/flash_controller_inst/u_Wishbone_Master_Top_256K/u_Flash_Ctroller_256K/u_ER_UFM/ | 4.822 | 1.786(0.000) | 3.036(0.000)
tb/flash_controller_inst/u_Wishbone_Master_Top_256K/u_Flash_Ctroller_256K/u_GW_USER_FLASH_256K/ | 1.764 | 0.219(0.000) | 1.545(0.000)
tb/flash_controller_inst/u_Wishbone_Master_Top_256K/u_Flash_Ctroller_256K/u_RD_UFM/ | 0.530 | 0.101(0.000) | 0.429(0.000)
tb/flash_controller_inst/u_Wishbone_Master_Top_256K/u_Flash_Ctroller_256K/u_WR_UFM/ | 4.624 | 1.545(0.000) | 3.079(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
DEFAULT_CLK | 100.000 | 20.189