Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH608K_REG_IF\project\impl\synthesize\rev_1\FLASH608K_REG_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH608K_REG_IF\project\src\FLASH608K_REG_IF.cst
Timing Constraints File | ---
GOWIN Version | V1.9.2.01Beta
Part Number | GW1N-LV9LQ144C6/I5
Created Time | Tue Oct 22 17:13:08 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 24.739
Quiescent Power (mW) | 4.491
Dynamic Power (mW) | 20.247

## Thermal Information:

Junction Temperature | 25.246
Theta JA | 10.100
Max Allowed Ambient Temperature | 84.750

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 15.050 | 2.523 | 21.088
VCCX | 2.500 | 0.509 | 0.341 | 2.125
VCCO18 | 1.800 | 0.508 | 0.340 | 1.526

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 4.331 | NA | 12.500
IO | 4.670 | 1.872 | 14.931

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
tb | 17.422 | 4.331(4.207) | 13.091(12.263)
tb/Gowin_Flash_Controller_template/ | 16.470 | 4.207(4.207) | 12.263(12.263)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_608K/ | 16.470 | 4.207(3.791) | 12.263(9.299)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_608K/u_ER_UFM/ | 5.023 | 1.794(0.000) | 3.228(0.000)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_608K/u_GW_USER_FLASH_608K/ | 2.391 | 0.224(0.000) | 2.166(0.000)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_608K/u_RD_UFM/ | 0.973 | 0.217(0.000) | 0.756(0.000)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_608K/u_WR_UFM/ | 4.703 | 1.555(0.000) | 3.148(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
DEFAULT_CLK | 100.000 | 17.449