Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH64KZ_REG_IF\project\impl\synthesize\rev_1\FLASH64KZ_REG_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH64KZ_REG_IF\project\src\FLASH64KZ_REG_IF.cst
Timing Constraints File | ---
GOWIN Version | V1.9.2.01Beta
Part Number | GW1NZ-ZV1FN32C5/I4
Created Time | Tue Oct 22 17:02:22 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 13.142
Quiescent Power (mW) | 1.370
Dynamic Power (mW) | 11.772

## Thermal Information:

Junction Temperature | 25.193
Theta JA | 14.800
Max Allowed Ambient Temperature | 84.805

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 0.900 | 12.287 | 1.153 | 12.096
VCCX | 1.800 | 0.198 | 0.092 | 0.523
VCCO18 | 1.800 | 0.198 | 0.092 | 0.523

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 3.084 | NA | 12.500
IO | 1.311 | 0.417 | 19.792

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
tb | 10.853 | 3.084(3.016) | 7.770(7.334)
tb/Gowin_Flash_Controller_template/ | 10.350 | 3.016(3.016) | 7.334(7.334)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_64K/ | 10.350 | 3.016(2.667) | 7.334(5.628)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_64K/u_ER_UFM_64K/ | 3.634 | 1.334(0.000) | 2.300(0.000)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_64K/u_GW_USER_FLASH_64K/ | 0.714 | 0.113(0.000) | 0.602(0.000)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_64K/u_RD_UFM_64K/ | 0.359 | 0.070(0.000) | 0.289(0.000)
tb/Gowin_Flash_Controller_template/u_Flash_Ctroller_64K/u_WR_UFM_64K/ | 3.587 | 1.150(0.000) | 2.437(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
DEFAULT_CLK | 100.000 | 10.878