Selecting top level module NLMS_Adaptive_Filter_Top
Running optimization stage 1 on \(divider)/(NLMS_Adaptive_Filter_Top) .......
Running optimization stage 1 on \(inv_nlms)/(NLMS_Adaptive_Filter_Top) .......
Running optimization stage 1 on \(pre_coe)/(NLMS_Adaptive_Filter_Top) .......
Running optimization stage 1 on \(coeffi_ctr)/(NLMS_Adaptive_Filter_Top)_36s_32s_5s .......
Running optimization stage 1 on \(data_ctr)/(NLMS_Adaptive_Filter_Top)_18s_32s_5s .......
Running optimization stage 1 on \(mult_accu)/(NLMS_Adaptive_Filter_Top)_36s_18s .......
Running optimization stage 1 on \(mult_accu)/(NLMS_Adaptive_Filter_Top)_18s_18s .......
Running optimization stage 1 on \(NLMS_top)/(NLMS_Adaptive_Filter_Top) .......
@N: CG364 :"C:\Gowin\1.8\IDE\ipcore\NLMS\data\NLMS_Adaptive_Filter_wrap.v":3:19:3:19|Synthesizing module NLMS_Adaptive_Filter_Top in library work.
Running optimization stage 1 on NLMS_Adaptive_Filter_Top .......
Running optimization stage 2 on NLMS_Adaptive_Filter_Top .......
Running optimization stage 2 on \(NLMS_top)/(NLMS_Adaptive_Filter_Top) .......
Running optimization stage 2 on \(mult_accu)/(NLMS_Adaptive_Filter_Top)_18s_18s .......
Running optimization stage 2 on \(mult_accu)/(NLMS_Adaptive_Filter_Top)_36s_18s .......
Running optimization stage 2 on \(data_ctr)/(NLMS_Adaptive_Filter_Top)_18s_32s_5s .......
Running optimization stage 2 on \(coeffi_ctr)/(NLMS_Adaptive_Filter_Top)_36s_32s_5s .......
Running optimization stage 2 on \(pre_coe)/(NLMS_Adaptive_Filter_Top) .......
Running optimization stage 2 on \(inv_nlms)/(NLMS_Adaptive_Filter_Top) .......
Running optimization stage 2 on \(divider)/(NLMS_Adaptive_Filter_Top) .......

For a summary of runtime and memory usage per design unit, please see file:
==========================================================
@L: E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\synwork\layer0.rt.csv

