@N: CG364 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\impl\gao\ao_0\gw_ao_parameter.v":1:0:1:8|Synthesizing module work_E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\impl\gao\ao_0\gw_ao_parameter.v_unit in library work.
Selecting top level module ao_top_0
Running optimization stage 1 on ao_mem_ctrl_0_1024s_33s_10s .......
Running optimization stage 1 on ao_crc32_0 .......
Running optimization stage 1 on ao_match_0_0s_1s_33s_0_1_0_1_2_3_4 .......
Running optimization stage 1 on ao_match_0_0s_13s_33s_0_1_0_1_2_3_4 .......
Running optimization stage 1 on ao_top_0 .......
Running optimization stage 2 on ao_match_0_0s_13s_33s_0_1_0_1_2_3_4 .......
Running optimization stage 2 on ao_match_0_0s_1s_33s_0_1_0_1_2_3_4 .......
Running optimization stage 2 on ao_top_0 .......
Extracted state machine for register module_state
State machine has 11 reachable states with original encodings of:
   0000
   0001
   0010
   0011
   0100
   0101
   0110
   0111
   1001
   1010
   1011
Running optimization stage 2 on ao_crc32_0 .......
Running optimization stage 2 on ao_mem_ctrl_0_1024s_33s_10s .......

For a summary of runtime and memory usage per design unit, please see file:
==========================================================
@L: E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\impl\gao\ao_0\rev_1\synwork\layer0.rt.csv

