@P:  Worst Slack : -0.990
@P:  NLMS_Adaptive_Filter_Top|clk - Estimated Frequency : 151.5 MHz
@P:  NLMS_Adaptive_Filter_Top|clk - Requested Frequency : 178.3 MHz
@P:  NLMS_Adaptive_Filter_Top|clk - Estimated Period : 6.599
@P:  NLMS_Adaptive_Filter_Top|clk - Requested Period : 5.609
@P:  NLMS_Adaptive_Filter_Top|clk - Slack : -0.990
@P:  System - Estimated Frequency : 563.3 MHz
@P:  System - Requested Frequency : 150.0 MHz
@P:  System - Estimated Period : 1.775
@P:  System - Requested Period : 6.667
@P:  System - Slack : 4.891
@P: NLMS_Adaptive_Filter_Top Part : gw2a_55pbga484-8
@P: NLMS_Adaptive_Filter_Top I/O Register bits : 0
@P: NLMS_Adaptive_Filter_Top Register bits (Non I/O) : 1045 (2%)
@P: NLMS_Adaptive_Filter_Top Block Rams : 2 of 140 (1%)
@P: NLMS_Adaptive_Filter_Top Total Luts : 805 of 800 (1%)
@P:  CPU Time : 0h:00m:32s
