Selecting top level module ALU54D
@N: CG364 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":859:7:859:12|Synthesizing module ALU54D in library work.
@W: CG532 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":890:4:890:10|Within an initial block, only Verilog force statements and memory $readmemh/$readmemb initialization statements are recognized, and all other content is ignored.
Running optimization stage 1 on ALU54D .......
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":1175:4:1175:9|Pruning unused register dout_reg_async[54:0]. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":1086:4:1086:9|Pruning unused register accload0_reg_sync. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":1072:4:1072:9|Pruning unused register accload0_reg_async. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":1047:4:1047:9|Pruning unused register bsign0_reg0_sync. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":1033:4:1033:9|Pruning unused register bsign0_reg0_async. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":1008:4:1008:9|Pruning unused register asign0_reg0_sync. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":994:4:994:9|Pruning unused register asign0_reg0_async. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":970:4:970:9|Pruning unused register inb0_reg_sync[53:0]. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":956:4:956:9|Pruning unused register inb0_reg_async[53:0]. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":932:4:932:9|Pruning unused register ina0_reg_sync[53:0]. Make sure that there are no unused intermediate registers.
@W: CL169 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":918:4:918:9|Pruning unused register ina0_reg_async[53:0]. Make sure that there are no unused intermediate registers.
Running optimization stage 2 on ALU54D .......
@N: CL159 :"E:\IP_PROJECT\NLMS\RefDesign_03_04\NLMS_REF_03_04\Gowin_NLMS_Adaptive_Filter_RefDesign\project\src\nlms_adaptive_filter\temp\NLMS_Adaptive_Filter\rev_1\syntmp\ALU54D.v":863:13:863:16|Input CASI is unused.
