@N: CG364 :"C:\Users\Noa\Desktop\Myworkplace\Program\FPGAProgram\Ref_design\src\pdm2pcm\temp\pdm2pcm\parameter.v":1:0:1:8|Synthesizing module work_C:\Users\Noa\Documents\WXWork\1688853129516911\Cache\File\2019-11\Gowin_V1.9.3Beta_36338_20191119\IDE\ipcore\PDM2PCM\data\pdm2pcm_wrap.v_unit in library work.
Selecting top level module PDM2PCM_Top
Running optimization stage 1 on \~syn_signal.PDM2PCM_Top  .......
Running optimization stage 1 on \~delay.PDM2PCM_Top _4s_2s .......
Running optimization stage 1 on PLL .......
Running optimization stage 1 on \~Gowin_PLL.PDM2PCM_Top  .......
Running optimization stage 1 on \~clk_div_even.PDM2PCM_Top  .......
Running optimization stage 1 on \~edge_detect.PDM2PCM_Top _1_4s .......
Running optimization stage 1 on \~parallel2series.PDM2PCM_Top _1_4s_4s_1s_2s .......
Running optimization stage 1 on \~cic_down_sample.PDM2PCM_Top _4s_32s_46s_2s .......
Running optimization stage 1 on \~data_round.PDM2PCM_Top _46s_24s_22s_23s_47s_0s .......
Running optimization stage 1 on \~data_round.PDM2PCM_Top _46s_46s_0s_45s_47s_0s .......
Running optimization stage 1 on \~cic_integrator.PDM2PCM_Top _4s_46s_46s .......
Running optimization stage 1 on \~cic_comb.PDM2PCM_Top _4s_1s_46s_46s_2s .......
Running optimization stage 1 on \~cic_decimator.PDM2PCM_Top _4s_64s_3s_1s_24s_24s_46s .......
Running optimization stage 1 on \~cic_filter.PDM2PCM_Top _4s_64s_3s_1s_24s_24s .......
Opening data file ./cic_comp_coeff.dat from directory C:\Users\Noa\Desktop\Myworkplace\Program\FPGAProgram\Ref_design\src\pdm2pcm\temp\pdm2pcm\.
Running optimization stage 1 on \~cic_cmp_rom.PDM2PCM_Top _96s_24s .......
Running optimization stage 1 on SDP .......
Running optimization stage 1 on \~Gowin_SDP.PDM2PCM_Top  .......
Running optimization stage 1 on \~delay.PDM2PCM_Top _6s_3s .......
Running optimization stage 1 on \~delay.PDM2PCM_Top _2s_5s .......
Running optimization stage 1 on \~delay.PDM2PCM_Top _6s_2s .......
Running optimization stage 1 on \~delay.PDM2PCM_Top _1s_59s .......
Running optimization stage 1 on \~data_round.PDM2PCM_Top _48s_24s_9s_23s_34s_15s .......
Running optimization stage 1 on \~cic_compensation_filter.PDM2PCM_Top _Z1 .......
Running optimization stage 1 on \~pdm2pcm.PDM2PCM_Top _96s_64s_3s_1s_4s_1_24s_24s_24s_4s .......
@N: CG364 :"C:\Users\Noa\Documents\WXWork\1688853129516911\Cache\File\2019-11\Gowin_V1.9.3Beta_36338_20191119\IDE\ipcore\PDM2PCM\data\pdm2pcm_wrap.v":4:19:4:19|Synthesizing module PDM2PCM_Top in library work.
Running optimization stage 1 on PDM2PCM_Top .......
Running optimization stage 2 on PDM2PCM_Top .......
Running optimization stage 2 on \~pdm2pcm.PDM2PCM_Top _96s_64s_3s_1s_4s_1_24s_24s_24s_4s .......
Running optimization stage 2 on \~cic_compensation_filter.PDM2PCM_Top _Z1 .......
Running optimization stage 2 on \~data_round.PDM2PCM_Top _48s_24s_9s_23s_34s_15s .......
Running optimization stage 2 on \~delay.PDM2PCM_Top _1s_59s .......
Running optimization stage 2 on \~delay.PDM2PCM_Top _6s_2s .......
Running optimization stage 2 on \~delay.PDM2PCM_Top _2s_5s .......
Running optimization stage 2 on \~delay.PDM2PCM_Top _6s_3s .......
Running optimization stage 2 on \~Gowin_SDP.PDM2PCM_Top  .......
Running optimization stage 2 on SDP .......
Running optimization stage 2 on \~cic_cmp_rom.PDM2PCM_Top _96s_24s .......
Running optimization stage 2 on \~cic_filter.PDM2PCM_Top _4s_64s_3s_1s_24s_24s .......
Running optimization stage 2 on \~cic_comb.PDM2PCM_Top _4s_1s_46s_46s_2s .......
Running optimization stage 2 on \~cic_integrator.PDM2PCM_Top _4s_46s_46s .......
Running optimization stage 2 on \~data_round.PDM2PCM_Top _46s_46s_0s_45s_47s_0s .......
Running optimization stage 2 on \~cic_decimator.PDM2PCM_Top _4s_64s_3s_1s_24s_24s_46s .......
Running optimization stage 2 on \~data_round.PDM2PCM_Top _46s_24s_22s_23s_47s_0s .......
Running optimization stage 2 on \~cic_down_sample.PDM2PCM_Top _4s_32s_46s_2s .......
Running optimization stage 2 on \~parallel2series.PDM2PCM_Top _1_4s_4s_1s_2s .......
Running optimization stage 2 on \~edge_detect.PDM2PCM_Top _1_4s .......
Running optimization stage 2 on \~clk_div_even.PDM2PCM_Top  .......
Running optimization stage 2 on \~Gowin_PLL.PDM2PCM_Top  .......
Running optimization stage 2 on PLL .......
Running optimization stage 2 on \~delay.PDM2PCM_Top _4s_2s .......
Running optimization stage 2 on \~syn_signal.PDM2PCM_Top  .......

For a summary of runtime and memory usage per design unit, please see file:
==========================================================
@L: C:\Users\Noa\Desktop\Myworkplace\Program\FPGAProgram\Ref_design\src\pdm2pcm\temp\pdm2pcm\rev_1\synwork\layer0.rt.csv

