Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | E:\IP_verify\1.9.3\IP_web\Gowin_PDM2PCM_RefDesign\PDM2PCM_RefDesign\project\impl\synthesize\rev_1\Ref_design.vm
Physical Constraints File | E:\IP_verify\1.9.3\IP_web\Gowin_PDM2PCM_RefDesign\PDM2PCM_RefDesign\project\src\Top.cst
Timing Constraints File | ---
GOWIN Version | V1.9.3Beta
Part Number | GW1N-LV9LQ144C6/I5
Created Time | Mon Dec 16 17:06:24 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 32.126
Quiescent Power (mW) | 4.195
Dynamic Power (mW) | 27.930

## Thermal Information:

Junction Temperature | 25.321
Theta JA | 10.100
Max Allowed Ambient Temperature | 84.676

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 23.219 | 2.470 | 30.828
VCCX | 2.500 | 0.016 | 0.286 | 0.755
VCCO18 | 1.800 | 0.016 | 0.286 | 0.543

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 5.183 | NA | 4.872
IO | 1.660 | 1.575 | 0.667
PLL | 1.116 | NA | NA

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
Top | 27.844 | 6.299(6.191) | 21.545(21.468)
Top/PDM2PCM_Top/ | 27.659 | 6.191(6.191) | 21.468(21.468)
Top/PDM2PCM_Top/pdm2pcm/ | 27.659 | 6.191(6.191) | 21.468(21.468)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/ | 8.401 | 0.976(0.090) | 7.425(1.131)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/cic_cmp_rom/ | 0.345 | 0.000(0.000) | 0.345(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/data_round/ | 0.070 | 0.006(0.000) | 0.064(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/delay_cnt_chn_rd_dx2/ | 0.116 | 0.016(0.000) | 0.100(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/delay_cnt_tdm/ | 0.157 | 0.028(0.000) | 0.129(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/delay_cnt_tdm_d/ | 0.072 | 0.007(0.000) | 0.065(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/delay_obstart/ | 0.291 | 0.033(0.000) | 0.259(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_cmp/dmem/ | 0.169 | 0.000(0.000) | 0.169(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/ | 17.748 | 4.039(4.039) | 13.709(13.709)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/ | 17.748 | 4.039(4.039) | 13.709(13.709)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/cic_ds/ | 1.210 | 0.159(0.000) | 1.051(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/comb[0].genblk1.cic_comb/ | 2.401 | 0.591(0.000) | 1.810(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/comb[1].genblk1.cic_comb/ | 2.373 | 0.591(0.000) | 1.783(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/comb[2].genblk1.cic_comb/ | 2.341 | 0.591(0.000) | 1.750(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/data_round/ | 0.331 | 0.041(0.000) | 0.290(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/intg[0].genblk1.cic_intg/ | 2.593 | 0.624(0.000) | 1.969(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/intg[1].genblk1.cic_intg/ | 3.119 | 0.722(0.000) | 2.398(0.000)
Top/PDM2PCM_Top/pdm2pcm/cic_filter/cic_decimator/intg[2].genblk1.cic_intg/ | 3.379 | 0.722(0.000) | 2.658(0.000)
Top/PDM2PCM_Top/pdm2pcm/clk_div_PDM/ | 0.141 | 0.033(0.000) | 0.108(0.000)
Top/PDM2PCM_Top/pdm2pcm/delay_in_pdm_data/ | 0.041 | 0.004(0.000) | 0.036(0.000)
Top/PDM2PCM_Top/pdm2pcm/edge_detect/ | 0.069 | 0.008(0.000) | 0.061(0.000)
Top/PDM2PCM_Top/pdm2pcm/iSysClk/ | 1.140 | 1.116(0.000) | 0.024(0.000)
Top/PDM2PCM_Top/pdm2pcm/parallel2series/ | 0.111 | 0.013(0.000) | 0.098(0.000)
Top/PDM2PCM_Top/pdm2pcm/syn_signal/ | 0.009 | 0.001(0.000) | 0.008(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
PDM2PCM_Top/pdm2pcm/iSysClk/pll_inst/CLKOUT.default_gen_clk | 40.000 | 26.729
NO CLOCK DOMAIN | 0.000 | 0.000
PDM2PCM_Top/pdm2pcm/iSysClk/pll_inst/CLKIN.default_clk | 50.000 | 1.116