@P:  Worst Slack : -2.018
@P:  PDM2PCM_Top|clk - Estimated Frequency : 74.3 MHz
@P:  PDM2PCM_Top|clk - Requested Frequency : 87.4 MHz
@P:  PDM2PCM_Top|clk - Estimated Period : 13.457
@P:  PDM2PCM_Top|clk - Requested Period : 11.438
@P:  PDM2PCM_Top|clk - Slack : -2.018
@P:  _~Gowin_PLL_PDM2PCM_Top_|clkout_inferred_clock - Estimated Frequency : 191.4 MHz
@P:  _~Gowin_PLL_PDM2PCM_Top_|clkout_inferred_clock - Requested Frequency : 225.2 MHz
@P:  _~Gowin_PLL_PDM2PCM_Top_|clkout_inferred_clock - Estimated Period : 5.225
@P:  _~Gowin_PLL_PDM2PCM_Top_|clkout_inferred_clock - Requested Period : 4.441
@P:  _~Gowin_PLL_PDM2PCM_Top_|clkout_inferred_clock - Slack : -0.784
@P:  System - Estimated Frequency : 191.6 MHz
@P:  System - Requested Frequency : 225.5 MHz
@P:  System - Estimated Period : 5.218
@P:  System - Requested Period : 4.435
@P:  System - Slack : -0.783
@P: PDM2PCM_Top Part : gw1n_9lqfp144-6
@P: PDM2PCM_Top I/O Register bits : 0
@P: PDM2PCM_Top Register bits (Non I/O) : 1210 (18%)
@P: PDM2PCM_Top Block Rams : 4 of 26 (15%)
@P: PDM2PCM_Top Total Luts : 1232 of 800 (14%)
@P:  CPU Time : 0h:00m:34s
