Project Status Summary Page

Project Settings
Project Name | pdm2pcm | Device Name | rev_1: GOWIN-GW1N : GW1N_9
Implementation Name | rev_1 | Top Module | [auto]
Pipelining | 1 | Retiming | 0
Resource Sharing | 1 | Fanout Guide | 10000
Disable I/O Insertion | 1 | Disable Sequential Optimizations | 0
Clock Conversion | 1 | FSM Compiler | 1

Run Status
Job Name | Status |  |  |  | CPU Time | Real Time | Memory | Date/Time
(compiler) | Complete | 9 | 4 | 0 | - | 00m:05s | - | 12/2/2019 10:15:39 AM
(premap) | Complete | 5 | 0 | 0 | 0m:02s | 0m:02s | 228MB | 12/2/2019 10:15:43 AM
(fpga_mapper) | Complete | 25 | 206 | 0 | 0m:34s | 0m:35s | 263MB | 12/2/2019 10:16:19 AM
Multi-srs Generator | Complete |  |  |  | 00m:01s |  |  | 12/2/2019 10:15:41 AM

Area Summary
Non I/O Register bits (non_io_reg) | 1210 (18%) | I/O Register bits (total_io_reg) | 0
Ultra Rams | 0 | Block Rams (v_ram) | 4 (26)
Block Multipliers (dsp_used) | 4 (10) | LUTs (total_luts) | 1232 (14%)

Timing Summary
Clock Name | Req Freq | Est Freq | Slack
--- | --- | --- | ---
PDM2PCM_Top|clk | 87.4 MHz | 74.3 MHz | -2.018
_~Gowin_PLL_PDM2PCM_Top_|clkout_inferred_clock | 225.2 MHz | 191.4 MHz | -0.784
System | 225.5 MHz | 191.6 MHz | -0.783

Optimizations Summary
Combined Clock Conversion | 1 / 1 |  |