@N: CG364 :"E:\W-File\PDM2PCM\RefDesign\project\Ref_design\temp\gao\ao_0\gw_ao_parameter.v":1:0:1:8|Synthesizing module work_E:\W-File\PDM2PCM\RefDesign\project\Ref_design\temp\gao\ao_0\gw_ao_parameter.v_unit in library work.
Selecting top level module ao_top
Running optimization stage 1 on ao_mem_ctrl_1024s_42s_10s .......
Running optimization stage 1 on ao_top .......
Running optimization stage 2 on ao_top .......
Extracted state machine for register module_state
State machine has 6 reachable states with original encodings of:
   0000
   0001
   0010
   0011
   0100
   0101
Running optimization stage 2 on ao_mem_ctrl_1024s_42s_10s .......

For a summary of runtime and memory usage per design unit, please see file:
==========================================================
@L: E:\W-File\PDM2PCM\RefDesign\project\Ref_design\temp\gao\ao_0\rev_1\synwork\layer0.rt.csv

