Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Tool Version | v1.8.1.01Beta
Series, Device, Package, Speed, Operating Condition, Process | GW2A,GW2A-55,PBGA484,8,COMMERCIAL,TYPICAL
Design Name | TOP
Design File | E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Lossless_ex\project\impl\synthesize\rev_1\lossless_ex.vm
Constraint File | E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Lossless_ex\project\src\lossless_ex.cst
Power Report File | E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Lossless_ex\project\impl\pnr\lossless_ex.power.html
Created Time | Wed Sep 19 08:47:03 2018
Command Line | D:\Gowin\1.8\Pnr\bin\gowin.exe -do E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Lossless_ex\project\impl\pnr\cmd.do
Legal Announcement | Copyright (C)2014-2018 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | -1.#IO
Quiescent Power (mW) | -1.#IO
Dynamic Power (mW) | -1.#IO

## Thermal Information:

Junction Temperature | -1.#IO
Theta JA | 0.000
Max Allowed Ambient Temperature | -1.#IO

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | true
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_100
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | -1.#IO | -1.#IO | -1.#IO
VCCX | 2.500 | 0.000 | 0.000 | 0.000

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
IO | 0.000 | 0.000 | 22.500

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
TOP | -1.#IO | 0.000(0.000) | -1.#IO(-1.#IO)
TOP/GW_PLL_inst/ | -1.#IO | 0.000(0.000) | -1.#IO(0.000)
TOP/osc_inst/ | -1.#IO | 0.000(0.000) | -1.#IO(0.000)
TOP/u_RAM_based_shift_reg | -1.#IO | 0.000(0.000) | -1.#IO(-1.#IO)
TOP/u_RAM_based_shift_reg/u_RAM_based_shift_reg/ | -1.#IO | 0.000(0.000) | -1.#IO(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
GW_PLL_inst/pll_inst/CLKOUT.default_gen_clk | 180.000 | -1.#IO