@P:  Worst Slack : -0.211
@P:  RAM_based_shift_reg_top|clk - Estimated Frequency : 709.7 MHz
@P:  RAM_based_shift_reg_top|clk - Requested Frequency : 834.9 MHz
@P:  RAM_based_shift_reg_top|clk - Estimated Period : 1.409
@P:  RAM_based_shift_reg_top|clk - Requested Period : 1.198
@P:  RAM_based_shift_reg_top|clk - Slack : -0.211
@P: RAM_based_shift_reg_top Part : gw2a_55pbga484-8
@P: RAM_based_shift_reg_top I/O Register bits : 0
@P: RAM_based_shift_reg_top Register bits (Non I/O) : 3 (0%)
@P: RAM_based_shift_reg_top Block Rams : 1 of 140 (0%)
@P: RAM_based_shift_reg_top Total Luts : 11 of 800 (0%)
@P:  CPU Time : 0h:00m:02s
