#Build: Synplify Pro (R) O-2018.09G-Beta1, Build 019R, Sep  3 2018
#install: D:\Gowin\1.8\SynplifyPro
#OS: Windows 7 6.1
#Hostname: GW-SW-042

# Wed Sep 19 08:39:49 2018

#Implementation: rev_1


Copyright (C) 1994-2018 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: O-2018.09G-Beta1
Install: D:\Gowin\1.8\SynplifyPro
OS: Windows 6.1

Hostname: GW-SW-042

Implementation : rev_1
Synopsys HDL Compiler, Version comp2018q3p1, Build 019R, Built Sep  3 2018 10:06:59

@N|Running in 64-bit mode
###########################################################[

Copyright (C) 1994-2018 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: O-2018.09G-Beta1
Install: D:\Gowin\1.8\SynplifyPro
OS: Windows 6.1

Hostname: GW-SW-042

Implementation : rev_1
Synopsys Verilog Compiler, Version comp2018q3p1, Build 019R, Built Sep  3 2018 10:06:59

@N|Running in 64-bit mode
@N: CG1349 :	| Running Verilog Compiler in System Verilog mode

@N: CG1350 :	| Running Verilog Compiler in Multiple File Compilation Unit mode

@I::"D:\Gowin\1.8\SynplifyPro\lib\generic\gw2a.v" (library work)
@I::"D:\Gowin\1.8\SynplifyPro\lib\vlog\hypermods.v" (library __hyper__lib__)
@I::"D:\Gowin\1.8\SynplifyPro\lib\vlog\umr_capim.v" (library snps_haps)
@I::"D:\Gowin\1.8\SynplifyPro\lib\vlog\scemi_objects.v" (library snps_haps)
@I::"D:\Gowin\1.8\SynplifyPro\lib\vlog\scemi_pipes.svh" (library snps_haps)
@I::"E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\gw_ao_parameter.v" (library work)
@I::"E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\gw_ao_top_define.v" (library work)
@I::"E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\gw_ao_expression.v" (library work)
@I::"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_crc32.v" (library work)
@I::"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_define.v" (library work)
@I::"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_match.v" (library work)
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_match.v":109:9:109:26|Net match_m0_en_reg_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_match.v":110:9:110:26|Net match_m1_en_reg_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_match.v":111:9:111:26|Net match_m2_en_reg_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_match.v":112:9:112:27|Net match_ctl_en_reg_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_match.v":113:9:113:24|Net match_cnt_reg_wr is not declared.
@I::"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_mem_ctrl.v" (library work)
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_mem_ctrl.v":122:9:122:27|Net capture_length_zero is not declared.
@I::"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v" (library work)
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":500:9:500:20|Net start_reg_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":503:9:503:29|Net trig_level_max_reg_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":504:9:504:31|Net capture_mem_addr_max_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":505:9:505:31|Net capture_mem_addr_rem_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":506:9:506:30|Net capture_windows_num_wr is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1717:9:1717:18|Net match_en_0 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1718:9:1718:18|Net match_en_1 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1719:9:1719:18|Net match_en_2 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1720:9:1720:18|Net match_en_3 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1721:9:1721:18|Net match_en_4 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1722:9:1722:18|Net match_en_5 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1723:9:1723:18|Net match_en_6 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1724:9:1724:18|Net match_en_7 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1725:9:1725:18|Net match_en_8 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1726:9:1726:18|Net match_en_9 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1727:9:1727:19|Net match_en_10 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1728:9:1728:19|Net match_en_11 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1729:9:1729:19|Net match_en_12 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1730:9:1730:19|Net match_en_13 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1731:9:1731:19|Net match_en_14 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":1732:9:1732:19|Net match_en_15 is not declared.
@W: CG1337 :"D:\Gowin\1.8\IDE\data\ipcores\GAO\GW_AO_0\gw_ao_top.v":2213:9:2213:16|Net stop_reg is not declared.
Verilog syntax check successful!
@N: CG364 :"E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\gw_ao_parameter.v":1:0:1:8|Synthesizing module work_E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\gw_ao_parameter.v_unit in library work.
Selecting top level module ao_top_0
Running optimization stage 1 on ao_mem_ctrl_0_1024s_17s_10s .......
Running optimization stage 1 on ao_crc32_0 .......
Running optimization stage 1 on ao_match_0_0s_8s_17s_4_1_0_1_2_3_4 .......
Running optimization stage 1 on ao_top_0 .......
Running optimization stage 2 on ao_match_0_0s_8s_17s_4_1_0_1_2_3_4 .......
Running optimization stage 2 on ao_top_0 .......
Extracted state machine for register module_state
State machine has 11 reachable states with original encodings of:
   0000
   0001
   0010
   0011
   0100
   0101
   0110
   0111
   1001
   1010
   1011
Running optimization stage 2 on ao_crc32_0 .......
Running optimization stage 2 on ao_mem_ctrl_0_1024s_17s_10s .......

For a summary of runtime and memory usage per design unit, please see file:
==========================================================
@L: E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\rev_1\synwork\layer0.rt.csv


At c_ver Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 79MB peak: 88MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Wed Sep 19 08:39:50 2018

###########################################################]
###########################################################[

Copyright (C) 1994-2018 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: O-2018.09G-Beta1
Install: D:\Gowin\1.8\SynplifyPro
OS: Windows 6.1

Hostname: GW-SW-042

Implementation : rev_1
Synopsys Synopsys Netlist Linker, Version comp2018q3p1, Build 019R, Built Sep  3 2018 10:06:59

@N|Running in 64-bit mode

At syn_nfilter Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 68MB peak: 69MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Wed Sep 19 08:39:50 2018

###########################################################]
@END

At c_hdl Exit (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:00s; Memory used current: 3MB peak: 4MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Wed Sep 19 08:39:50 2018

###########################################################]
###########################################################[

Copyright (C) 1994-2018 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: O-2018.09G-Beta1
Install: D:\Gowin\1.8\SynplifyPro
OS: Windows 6.1

Hostname: GW-SW-042

Database state : E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\rev_1\synwork\|rev_1
Synopsys Synopsys Netlist Linker, Version comp2018q3p1, Build 019R, Built Sep  3 2018 10:06:59

@N|Running in 64-bit mode

At syn_nfilter Exit (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 68MB peak: 69MB)

Process took 0h:00m:01s realtime, 0h:00m:01s cputime

Process completed successfully.
# Wed Sep 19 08:39:52 2018

###########################################################]
Premap Report

# Wed Sep 19 08:39:52 2018


Copyright (C) 1994-2018 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: O-2018.09G-Beta1
Install: D:\Gowin\1.8\SynplifyPro
OS: Windows 6.1

Hostname: GW-SW-042

Implementation : rev_1
Synopsys Generic Technology Pre-mapping, Version mapgw, Build 1167R, Built Sep  4 2018 10:03:38


Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 100MB)

@A: MF827 |No constraint file specified.
@N: MF284 |Setting synthesis effort to medium for the design
@L: E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\rev_1\ao_0_scck.rpt 
Printing clock  summary report in "E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\rev_1\ao_0_scck.rpt" file 
@N: MF916 |Option synthesis_strategy=base is enabled. 
@N: MF248 |Running in 64-bit mode.
@N: MF666 |Clock conversion enabled. (Command "set_option -fix_gated_and_generated_clocks 1" in the project file.)

Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 101MB peak: 103MB)


Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 101MB peak: 103MB)

@N: BN133 |Ignoring syn_hier=hard property on top-level design.

Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 102MB peak: 103MB)


Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 114MB peak: 116MB)

@N: MF284 |Setting synthesis effort to medium for the design
@N: MH105 |UMR3 is only supported for HAPS-80.
@N: MH105 |UMR3 is only supported for HAPS-80.

Beginning opaque latch detection (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)


Finished opaque latch marking step (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)

Rerun analysis in 0 latches

Finished opaque latch detection step 2 (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)

@N: MF974 |Total number of latches (multibit) processed = 0 
@N: MF975 |Total number of latches (bit blasted) processed = 0 
@N: MF976 |Total number of (multibit) opaque latches found = 0 
@N: MF977 |Total number of (bit blasted) opaque latches found = 0 

Finished opaque latch detection (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)







Detailed report for transparent and observable latches in design:
@L: E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\rev_1\synwork\ao_0_prem_latch_transparency_report.log
Encoding state machine module_state[10:0] (in view: work.ao_top_0(verilog))
original code -> new code
   0000 -> 00000000001
   0001 -> 00000000010
   0010 -> 00000000100
   0011 -> 00000001000
   0100 -> 00000010000
   0101 -> 00000100000
   0110 -> 00001000000
   0111 -> 00010000000
   1001 -> 00100000000
   1010 -> 01000000000
   1011 -> 10000000000

Starting clock optimization phase (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)


Finished clock optimization phase (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)


Starting clock optimization report phase (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)


Finished clock optimization report phase (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)

syn_allowed_resources : blockrams=140  set on top level netlist ao_top_0

Finished netlist restructuring (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)



Clock Summary
******************

          Start                   Requested     Requested     Clock        Clock                     Clock
Level     Clock                   Frequency     Period        Type         Group                     Load 
----------------------------------------------------------------------------------------------------------
0 -       ao_top_0|control[0]     186.5 MHz     5.362         inferred     Autoconstr_clkgroup_1     268  
                                                                                                          
0 -       ao_top_0|clk_i          237.7 MHz     4.207         inferred     Autoconstr_clkgroup_0     75   
==========================================================================================================



Clock Load Summary
***********************

                        Clock     Source               Clock Pin                                Non-clock Pin     Non-clock Pin       
Clock                   Load      Pin                  Seq Example                              Seq Example       Comb Example        
--------------------------------------------------------------------------------------------------------------------------------------
ao_top_0|control[0]     268       control[0](port)     data_register[37:0].C                    -                 -                   
                                                                                                                                      
ao_top_0|clk_i          75        clk_i(port)          internal_reg_force_triger_syn[1:0].C     -                 clk_ao.I[0](keepbuf)
======================================================================================================================================


ICG Latch Removal Summary:
Number of ICG latches removed: 0
Number of ICG latches not removed:	0


@S |Clock Optimization Summary



#### START OF PREMAP CLOCK OPTIMIZATION REPORT #####[

2 non-gated/non-generated clock tree(s) driving 327 clock pin(s) of sequential element(s)
0 gated/generated clock tree(s) driving 0 clock pin(s) of sequential element(s)
0 instances converted, 0 sequential instances remain driven by gated/generated clocks

============================= Non-Gated/Non-Generated Clocks =============================
Clock Tree ID     Driving Element     Drive Element Type        Fanout     Sample Instance
------------------------------------------------------------------------------------------
@KP:ckid0_0       ENCRYPTED           Unconstrained_port        59         ENCRYPTED      
@KP:ckid0_1       ENCRYPTED           Unconstrained_io_port     268        ENCRYPTED      
==========================================================================================


##### END OF CLOCK OPTIMIZATION REPORT ######

@N: FX1143 |Skipping assigning INTERNAL_VREF to iobanks, because the table of mapping from pin to iobank is not initialized.
Finished Pre Mapping Phase.
@N: BN225 |Writing default property annotation file E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\rev_1\ao_0.sap.

Starting constraint checker (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 191MB peak: 193MB)


Finished constraint checker preprocessing (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 191MB peak: 193MB)

None
None

Finished constraint checker (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 192MB peak: 193MB)

Pre-mapping successful!

At Mapper Exit (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 107MB peak: 193MB)

Process took 0h:00m:02s realtime, 0h:00m:01s cputime
# Wed Sep 19 08:39:54 2018

###########################################################]
Map & Optimize Report

# Wed Sep 19 08:39:54 2018


Copyright (C) 1994-2018 Synopsys, Inc.
This Synopsys software and all associated documentation are proprietary to Synopsys, Inc.
and may only be used pursuant to the terms and conditions of a written license agreement
with Synopsys, Inc. All other use, reproduction, modification, or distribution of the
Synopsys software or the associated documentation is strictly prohibited.
Tool: Synplify Pro (R)
Build: O-2018.09G-Beta1
Install: D:\Gowin\1.8\SynplifyPro
OS: Windows 6.1

Hostname: GW-SW-042

Implementation : rev_1
Synopsys Generic Technology Mapper, Version mapgw, Build 1167R, Built Sep  4 2018 10:03:38


Mapper Startup Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 99MB peak: 100MB)

@N: MF284 |Setting synthesis effort to medium for the design
@N: MF916 |Option synthesis_strategy=base is enabled. 
@N: MF248 |Running in 64-bit mode.
@N: MF666 |Clock conversion enabled. (Command "set_option -fix_gated_and_generated_clocks 1" in the project file.)

Design Input Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 98MB peak: 100MB)


Mapper Initialization Complete (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 98MB peak: 100MB)


Start loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 101MB peak: 102MB)


Finished loading timing files (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 113MB peak: 115MB)

@N: MF284 |Setting synthesis effort to medium for the design


Starting Optimization and Mapping (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 191MB peak: 192MB)


Available hyper_sources - for debug and ip models
	None Found

@N: MT206 |Auto Constrain mode is enabled

Finished RTL optimizations (Real Time elapsed 0h:00m:00s; CPU Time elapsed 0h:00m:00s; Memory used current: 190MB peak: 192MB)


Starting factoring (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 193MB peak: 194MB)


Finished factoring (Real Time elapsed 0h:00m:01s; CPU Time elapsed 0h:00m:01s; Memory used current: 201MB peak: 202MB)


Finished generic timing optimizations - Pass 1 (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 198MB peak: 202MB)


Starting Early Timing Optimization (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 198MB peak: 202MB)


Finished Early Timing Optimization (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:01s; Memory used current: 198MB peak: 202MB)


Finished generic timing optimizations - Pass 2 (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 198MB peak: 202MB)


Finished preparing to map (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 198MB peak: 202MB)


Finished technology mapping (Real Time elapsed 0h:00m:02s; CPU Time elapsed 0h:00m:02s; Memory used current: 220MB peak: 222MB)

Pass		 CPU time		Worst Slack		Luts / Registers
------------------------------------------------------------
   1		0h:00m:02s		    -2.87ns		 465 /       303
   2		0h:00m:02s		    -2.87ns		 468 /       303
   3		0h:00m:02s		    -2.60ns		 468 /       303
Timing driven replication report
Added 1 Registers via timing driven replication
Added 1 LUTs via timing driven replication

   4		0h:00m:03s		    -2.46ns		 490 /       304
   5		0h:00m:03s		    -2.73ns		 491 /       304
   6		0h:00m:03s		    -2.60ns		 491 /       304
   7		0h:00m:03s		    -2.60ns		 491 /       304
   8		0h:00m:03s		    -2.73ns		 492 /       304


   9		0h:00m:03s		    -2.46ns		 491 /       304

Finished technology timing optimizations and critical path resynthesis (Real Time elapsed 0h:00m:03s; CPU Time elapsed 0h:00m:03s; Memory used current: 222MB peak: 223MB)

@N: FX164 |The option to pack registers in the IOB has not been specified. Please set syn_useioff attribute.  

Finished restoring hierarchy (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:03s; Memory used current: 222MB peak: 223MB)


Start Writing Netlists (Real Time elapsed 0h:00m:04s; CPU Time elapsed 0h:00m:04s; Memory used current: 151MB peak: 223MB)

Writing Analyst data base E:\ide\IP_TEST_GOLDEN\gwip_ref_design\gwip_ref_design\Gowin_RAM_Based_Shift_Register_IP_RefDesign\Fixed_ex\project\impl\temp\gao\ao_0\rev_1\synwork\ao_0_m.srm

Finished Writing Netlist Databases (Real Time elapsed 0h:00m:05s; CPU Time elapsed 0h:00m:04s; Memory used current: 220MB peak: 223MB)

Writing Verilog Simulation files

Writing scf file... (Real Time elapsed 0h:00m:06s; CPU Time elapsed 0h:00m:05s; Memory used current: 220MB peak: 223MB)

@N: BW103 |The default time unit for the Synopsys Constraint File (SDC or FDC) is 1ns.
@N: BW107 |Synopsys Constraint File capacitance units using default value of 1pF 

Finished Writing Verilog Simulation files (Real Time elapsed 0h:00m:06s; CPU Time elapsed 0h:00m:05s; Memory used current: 219MB peak: 223MB)


Start final timing analysis (Real Time elapsed 0h:00m:06s; CPU Time elapsed 0h:00m:06s; Memory used current: 220MB peak: 223MB)

@W: MT420 |Found inferred clock ao_top_0|clk_i with period 4.43ns. Please declare a user-defined clock on port clk_i.
@W: MT420 |Found inferred clock ao_top_0|control[0] with period 6.21ns. Please declare a user-defined clock on port control[0].


##### START OF TIMING REPORT #####[
# Timing Report written on Wed Sep 19 08:40:01 2018
#


Top view:               ao_top_0
Requested Frequency:    161.0 MHz
Wire load mode:         top
Paths requested:        5
Constraint File(s):    
@N: MT320 |This timing report is an estimate of place and route data. For final timing results, use the FPGA vendor place and route report.

@N: MT322 |Clock constraints include only register-to-register paths associated with each individual clock.



Performance Summary
*******************


Worst slack in design: -1.096

                        Requested     Estimated     Requested     Estimated                Clock        Clock                
Starting Clock          Frequency     Frequency     Period        Period        Slack      Type         Group                
-----------------------------------------------------------------------------------------------------------------------------
ao_top_0|clk_i          225.9 MHz     192.0 MHz     4.426         5.207         -0.781     inferred     Autoconstr_clkgroup_0
ao_top_0|control[0]     161.0 MHz     136.8 MHz     6.212         7.309         -1.096     inferred     Autoconstr_clkgroup_1
System                  150.0 MHz     228.2 MHz     6.667         4.382         2.284      system       system_clkgroup      
=============================================================================================================================





Clock Relationships
*******************

Clocks                                    |    rise  to  rise    |    fall  to  fall   |    rise  to  fall   |    fall  to  rise 
---------------------------------------------------------------------------------------------------------------------------------
Starting             Ending               |  constraint  slack   |  constraint  slack  |  constraint  slack  |  constraint  slack
---------------------------------------------------------------------------------------------------------------------------------
System               ao_top_0|clk_i       |  4.426       2.284   |  No paths    -      |  No paths    -      |  No paths    -    
System               ao_top_0|control[0]  |  6.212       4.296   |  No paths    -      |  No paths    -      |  No paths    -    
ao_top_0|clk_i       System               |  4.426       3.648   |  No paths    -      |  No paths    -      |  No paths    -    
ao_top_0|clk_i       ao_top_0|clk_i       |  4.426       -0.781  |  4.426       3.587  |  No paths    -      |  2.213       1.374
ao_top_0|clk_i       ao_top_0|control[0]  |  Diff grp    -       |  No paths    -      |  No paths    -      |  No paths    -    
ao_top_0|control[0]  System               |  6.212       5.251   |  No paths    -      |  No paths    -      |  No paths    -    
ao_top_0|control[0]  ao_top_0|clk_i       |  Diff grp    -       |  No paths    -      |  No paths    -      |  No paths    -    
ao_top_0|control[0]  ao_top_0|control[0]  |  6.212       -1.096  |  No paths    -      |  No paths    -      |  No paths    -    
=================================================================================================================================
 Note: 'No paths' indicates there are no paths in the design for that pair of clock edges.
       'Diff grp' indicates that paths exist but the starting clock and ending clock are in different clock groups.



Interface Information 
*********************

No IO constraint found



====================================
Detailed Report for Clock: ao_top_0|clk_i
====================================



Starting Points with Worst Slack
********************************

                                     Starting                                                                 Arrival           
Instance                             Reference          Type     Pin     Net                                  Time        Slack 
                                     Clock                                                                                      
--------------------------------------------------------------------------------------------------------------------------------
triger_level_cnt[3]                  ao_top_0|clk_i     DFFC     Q       triger_level_cnt[3]                  0.243       -0.781
triger_level_cnt[2]                  ao_top_0|clk_i     DFFC     Q       triger_level_cnt[2]                  0.243       -0.760
capture_window_sel[2]                ao_top_0|clk_i     DFFC     Q       capture_window_sel[2]                0.243       -0.720
internal_reg_force_triger_syn[1]     ao_top_0|clk_i     DFFC     Q       internal_reg_force_triger_syn[1]     0.243       -0.716
capture_window_sel[0]                ao_top_0|clk_i     DFFC     Q       capture_window_sel[0]                0.243       -0.699
genblk1\.u_ao_match_0.match_sep      ao_top_0|clk_i     DFFC     Q       match                                0.243       -0.695
capture_window_sel[1]                ao_top_0|clk_i     DFFC     Q       capture_window_sel[1]                0.243       -0.608
triger_level_cnt[0]                  ao_top_0|clk_i     DFFC     Q       triger_level_cnt[0]                  0.243       -0.608
triger_level_cnt[1]                  ao_top_0|clk_i     DFFC     Q       triger_level_cnt[1]                  0.243       -0.517
u_ao_mem_ctrl.capture_length[0]      ao_top_0|clk_i     DFFC     Q       capture_length[0]                    0.243       -0.414
================================================================================================================================


Ending Points with Worst Slack
******************************

                                    Starting                                                       Required           
Instance                            Reference          Type      Pin     Net                       Time         Slack 
                                    Clock                                                                             
----------------------------------------------------------------------------------------------------------------------
u_ao_mem_ctrl.capture_mem_wr        ao_top_0|clk_i     DFFCE     CE      un1_start_reg             4.365        -0.781
u_ao_mem_ctrl.mem_addr_inc_en       ao_top_0|clk_i     DFFCE     CE      mem_addr_inc_en_RNO       4.365        -0.690
u_ao_mem_ctrl.mem_addr_inc_en       ao_top_0|clk_i     DFFCE     D       mem_addr_inc_en7          4.365        -0.117
triger_level_cnt[2]                 ao_top_0|clk_i     DFFC      D       triger_level_cnt_4[2]     4.365        -0.056
u_ao_mem_ctrl.capture_length[0]     ao_top_0|clk_i     DFFC      D       capture_length_5[0]       4.365        -0.009
u_ao_mem_ctrl.capture_length[1]     ao_top_0|clk_i     DFFC      D       capture_length_5[1]       4.365        -0.009
u_ao_mem_ctrl.capture_length[2]     ao_top_0|clk_i     DFFC      D       capture_length_5[2]       4.365        -0.009
u_ao_mem_ctrl.capture_length[3]     ao_top_0|clk_i     DFFP      D       capture_length_5[3]       4.365        -0.009
u_ao_mem_ctrl.capture_length[4]     ao_top_0|clk_i     DFFC      D       capture_length_5[4]       4.365        -0.009
u_ao_mem_ctrl.capture_length[5]     ao_top_0|clk_i     DFFC      D       capture_length_5[5]       4.365        -0.009
======================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      4.426
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         4.365

    - Propagation time:                      5.146
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.781

    Number of logic level(s):                5
    Starting point:                          triger_level_cnt[3] / Q
    Ending point:                            u_ao_mem_ctrl.capture_mem_wr / CE
    The start point is clocked by            ao_top_0|clk_i [rising] on pin CLK
    The end   point is clocked by            ao_top_0|clk_i [rising] on pin CLK

Instance / Net                              Pin      Pin               Arrival     No. of    
Name                              Type      Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------------------
triger_level_cnt[3]               DFFC      Q        Out     0.243     0.243       -         
triger_level_cnt[3]               Net       -        -       0.535     -           4         
triger_level_cnt13_1              LUT2      I1       In      -         0.778       -         
triger_level_cnt13_1              LUT2      F        Out     0.570     1.348       -         
triger_level_cnt13_1              Net       -        -       0.401     -           1         
triger_level_cnt13                LUT4      I1       In      -         1.749       -         
triger_level_cnt13                LUT4      F        Out     0.570     2.319       -         
triger_level_cnt13                Net       -        -       0.535     -           5         
triger_level_cnt_0_sqmuxa         LUT3      I2       In      -         2.854       -         
triger_level_cnt_0_sqmuxa         LUT3      F        Out     0.462     3.316       -         
triger_level_cnt_0_sqmuxa         Net       -        -       0.596     -           15        
u_ao_mem_ctrl.un1_start_reg_1     LUT4      I2       In      -         3.912       -         
u_ao_mem_ctrl.un1_start_reg_1     LUT4      F        Out     0.462     4.374       -         
un1_start_reg_1                   Net       -        -       0.401     -           1         
u_ao_mem_ctrl.un1_start_reg       LUT4      I3       In      -         4.775       -         
u_ao_mem_ctrl.un1_start_reg       LUT4      F        Out     0.371     5.146       -         
un1_start_reg                     Net       -        -       0.000     -           1         
u_ao_mem_ctrl.capture_mem_wr      DFFCE     CE       In      -         5.146       -         
=============================================================================================
Total path delay (propagation time + setup) of 5.207 is 2.739(52.6%) logic and 2.468(47.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 2: 
      Requested Period:                      4.426
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         4.365

    - Propagation time:                      5.125
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.760

    Number of logic level(s):                5
    Starting point:                          triger_level_cnt[2] / Q
    Ending point:                            u_ao_mem_ctrl.capture_mem_wr / CE
    The start point is clocked by            ao_top_0|clk_i [rising] on pin CLK
    The end   point is clocked by            ao_top_0|clk_i [rising] on pin CLK

Instance / Net                              Pin      Pin               Arrival     No. of    
Name                              Type      Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------------------
triger_level_cnt[2]               DFFC      Q        Out     0.243     0.243       -         
triger_level_cnt[2]               Net       -        -       0.535     -           5         
triger_level_cnt13_1              LUT2      I0       In      -         0.778       -         
triger_level_cnt13_1              LUT2      F        Out     0.549     1.327       -         
triger_level_cnt13_1              Net       -        -       0.401     -           1         
triger_level_cnt13                LUT4      I1       In      -         1.728       -         
triger_level_cnt13                LUT4      F        Out     0.570     2.298       -         
triger_level_cnt13                Net       -        -       0.535     -           5         
triger_level_cnt_0_sqmuxa         LUT3      I2       In      -         2.833       -         
triger_level_cnt_0_sqmuxa         LUT3      F        Out     0.462     3.295       -         
triger_level_cnt_0_sqmuxa         Net       -        -       0.596     -           15        
u_ao_mem_ctrl.un1_start_reg_1     LUT4      I2       In      -         3.891       -         
u_ao_mem_ctrl.un1_start_reg_1     LUT4      F        Out     0.462     4.353       -         
un1_start_reg_1                   Net       -        -       0.401     -           1         
u_ao_mem_ctrl.un1_start_reg       LUT4      I3       In      -         4.754       -         
u_ao_mem_ctrl.un1_start_reg       LUT4      F        Out     0.371     5.125       -         
un1_start_reg                     Net       -        -       0.000     -           1         
u_ao_mem_ctrl.capture_mem_wr      DFFCE     CE       In      -         5.125       -         
=============================================================================================
Total path delay (propagation time + setup) of 5.186 is 2.718(52.4%) logic and 2.468(47.6%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 3: 
      Requested Period:                      4.426
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         4.365

    - Propagation time:                      5.085
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.720

    Number of logic level(s):                5
    Starting point:                          capture_window_sel[2] / Q
    Ending point:                            u_ao_mem_ctrl.capture_mem_wr / CE
    The start point is clocked by            ao_top_0|clk_i [rising] on pin CLK
    The end   point is clocked by            ao_top_0|clk_i [rising] on pin CLK

Instance / Net                              Pin      Pin               Arrival     No. of    
Name                              Type      Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------------------
capture_window_sel[2]             DFFC      Q        Out     0.243     0.243       -         
capture_window_sel[2]             Net       -        -       0.535     -           5         
un6_start_reg_ac0_5_c_2           LUT4      I1       In      -         0.778       -         
un6_start_reg_ac0_5_c_2           LUT4      F        Out     0.570     1.348       -         
un6_start_reg_ac0_5_c_2           Net       -        -       0.401     -           1         
un6_start_reg_ac0_5_0_0           LUT4      I2       In      -         1.749       -         
un6_start_reg_ac0_5_0_0           LUT4      F        Out     0.462     2.211       -         
un6_start_reg_ac0_5_0_0           Net       -        -       0.535     -           2         
start_reg                         LUT4      I2       In      -         2.746       -         
start_reg                         LUT4      F        Out     0.462     3.208       -         
start_reg                         Net       -        -       0.535     -           4         
u_ao_mem_ctrl.un1_start_reg_1     LUT4      I1       In      -         3.743       -         
u_ao_mem_ctrl.un1_start_reg_1     LUT4      F        Out     0.570     4.313       -         
un1_start_reg_1                   Net       -        -       0.401     -           1         
u_ao_mem_ctrl.un1_start_reg       LUT4      I3       In      -         4.714       -         
u_ao_mem_ctrl.un1_start_reg       LUT4      F        Out     0.371     5.085       -         
un1_start_reg                     Net       -        -       0.000     -           1         
u_ao_mem_ctrl.capture_mem_wr      DFFCE     CE       In      -         5.085       -         
=============================================================================================
Total path delay (propagation time + setup) of 5.146 is 2.739(53.2%) logic and 2.407(46.8%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 4: 
      Requested Period:                      4.426
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         4.365

    - Propagation time:                      5.081
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.716

    Number of logic level(s):                5
    Starting point:                          internal_reg_force_triger_syn[1] / Q
    Ending point:                            u_ao_mem_ctrl.capture_mem_wr / CE
    The start point is clocked by            ao_top_0|clk_i [rising] on pin CLK
    The end   point is clocked by            ao_top_0|clk_i [rising] on pin CLK

Instance / Net                                 Pin      Pin               Arrival     No. of    
Name                                 Type      Name     Dir     Delay     Time        Fan Out(s)
------------------------------------------------------------------------------------------------
internal_reg_force_triger_syn[1]     DFFC      Q        Out     0.243     0.243       -         
internal_reg_force_triger_syn[1]     Net       -        -       0.535     -           1         
un1_match_final_3                    LUT4      I1       In      -         0.778       -         
un1_match_final_3                    LUT4      F        Out     0.570     1.348       -         
un1_match_final_3                    Net       -        -       0.535     -           2         
triger_level_cnt13                   LUT4      I3       In      -         1.883       -         
triger_level_cnt13                   LUT4      F        Out     0.371     2.254       -         
triger_level_cnt13                   Net       -        -       0.535     -           5         
triger_level_cnt_0_sqmuxa            LUT3      I2       In      -         2.789       -         
triger_level_cnt_0_sqmuxa            LUT3      F        Out     0.462     3.251       -         
triger_level_cnt_0_sqmuxa            Net       -        -       0.596     -           15        
u_ao_mem_ctrl.un1_start_reg_1        LUT4      I2       In      -         3.847       -         
u_ao_mem_ctrl.un1_start_reg_1        LUT4      F        Out     0.462     4.309       -         
un1_start_reg_1                      Net       -        -       0.401     -           1         
u_ao_mem_ctrl.un1_start_reg          LUT4      I3       In      -         4.710       -         
u_ao_mem_ctrl.un1_start_reg          LUT4      F        Out     0.371     5.081       -         
un1_start_reg                        Net       -        -       0.000     -           1         
u_ao_mem_ctrl.capture_mem_wr         DFFCE     CE       In      -         5.081       -         
================================================================================================
Total path delay (propagation time + setup) of 5.142 is 2.540(49.4%) logic and 2.602(50.6%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 5: 
      Requested Period:                      4.426
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         4.365

    - Propagation time:                      5.064
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (non-critical) :                 -0.699

    Number of logic level(s):                5
    Starting point:                          capture_window_sel[0] / Q
    Ending point:                            u_ao_mem_ctrl.capture_mem_wr / CE
    The start point is clocked by            ao_top_0|clk_i [rising] on pin CLK
    The end   point is clocked by            ao_top_0|clk_i [rising] on pin CLK

Instance / Net                              Pin      Pin               Arrival     No. of    
Name                              Type      Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------------------
capture_window_sel[0]             DFFC      Q        Out     0.243     0.243       -         
capture_window_sel[0]             Net       -        -       0.535     -           7         
un6_start_reg_ac0_5_c_2           LUT4      I0       In      -         0.778       -         
un6_start_reg_ac0_5_c_2           LUT4      F        Out     0.549     1.327       -         
un6_start_reg_ac0_5_c_2           Net       -        -       0.401     -           1         
un6_start_reg_ac0_5_0_0           LUT4      I2       In      -         1.728       -         
un6_start_reg_ac0_5_0_0           LUT4      F        Out     0.462     2.190       -         
un6_start_reg_ac0_5_0_0           Net       -        -       0.535     -           2         
start_reg                         LUT4      I2       In      -         2.725       -         
start_reg                         LUT4      F        Out     0.462     3.187       -         
start_reg                         Net       -        -       0.535     -           4         
u_ao_mem_ctrl.un1_start_reg_1     LUT4      I1       In      -         3.722       -         
u_ao_mem_ctrl.un1_start_reg_1     LUT4      F        Out     0.570     4.292       -         
un1_start_reg_1                   Net       -        -       0.401     -           1         
u_ao_mem_ctrl.un1_start_reg       LUT4      I3       In      -         4.693       -         
u_ao_mem_ctrl.un1_start_reg       LUT4      F        Out     0.371     5.064       -         
un1_start_reg                     Net       -        -       0.000     -           1         
u_ao_mem_ctrl.capture_mem_wr      DFFCE     CE       In      -         5.064       -         
=============================================================================================
Total path delay (propagation time + setup) of 5.125 is 2.718(53.0%) logic and 2.407(47.0%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value




====================================
Detailed Report for Clock: ao_top_0|control[0]
====================================



Starting Points with Worst Slack
********************************

                                 Starting                                                                   Arrival           
Instance                         Reference               Type      Pin     Net                              Time        Slack 
                                 Clock                                                                                        
------------------------------------------------------------------------------------------------------------------------------
internal_register_select[9]      ao_top_0|control[0]     DFFCE     Q       internal_register_select[9]      0.243       -1.096
internal_register_select[7]      ao_top_0|control[0]     DFFCE     Q       internal_register_select[7]      0.243       -1.075
internal_register_select[10]     ao_top_0|control[0]     DFFCE     Q       internal_register_select[10]     0.243       -0.988
internal_register_select[11]     ao_top_0|control[0]     DFFCE     Q       internal_register_select[11]     0.243       -0.897
word_count[13]                   ao_top_0|control[0]     DFFCE     Q       word_count[13]                   0.243       -0.792
word_count[1]                    ao_top_0|control[0]     DFFCE     Q       word_count[1]                    0.243       -0.771
word_count[10]                   ao_top_0|control[0]     DFFCE     Q       word_count[10]                   0.243       -0.771
word_count[0]                    ao_top_0|control[0]     DFFCE     Q       word_count[0]                    0.243       -0.750
word_count[3]                    ao_top_0|control[0]     DFFCE     Q       word_count[3]                    0.243       -0.684
word_count[14]                   ao_top_0|control[0]     DFFCE     Q       word_count[14]                   0.243       -0.684
==============================================================================================================================


Ending Points with Worst Slack
******************************

                          Starting                                                              Required           
Instance                  Reference               Type      Pin     Net                         Time         Slack 
                          Clock                                                                                    
-------------------------------------------------------------------------------------------------------------------
data_out_shift_reg[3]     ao_top_0|control[0]     DFFCE     D       data_out_shift_reg_4[3]     6.151        -1.096
data_out_shift_reg[4]     ao_top_0|control[0]     DFFCE     D       data_out_shift_reg_4[4]     6.151        -1.096
data_out_shift_reg[5]     ao_top_0|control[0]     DFFCE     D       data_out_shift_reg_4[5]     6.151        -1.096
data_out_shift_reg[6]     ao_top_0|control[0]     DFFCE     D       data_out_shift_reg_4[6]     6.151        -1.096
data_out_shift_reg[7]     ao_top_0|control[0]     DFFCE     D       data_out_shift_reg_4[7]     6.151        -1.096
data_out_shift_reg[1]     ao_top_0|control[0]     DFFCE     D       data_out_shift_reg_4[1]     6.151        -1.025
data_out_shift_reg[0]     ao_top_0|control[0]     DFFCE     D       data_out_shift_reg_4[0]     6.151        -0.955
address_counter[0]        ao_top_0|control[0]     DFFCE     CE      addr_ct_en                  6.151        -0.792
address_counter[1]        ao_top_0|control[0]     DFFCE     CE      addr_ct_en                  6.151        -0.792
address_counter[2]        ao_top_0|control[0]     DFFCE     CE      addr_ct_en                  6.151        -0.792
===================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      6.212
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         6.151

    - Propagation time:                      7.248
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (critical) :                     -1.096

    Number of logic level(s):                7
    Starting point:                          internal_register_select[9] / Q
    Ending point:                            data_out_shift_reg[4] / D
    The start point is clocked by            ao_top_0|control[0] [rising] on pin CLK
    The end   point is clocked by            ao_top_0|control[0] [rising] on pin CLK

Instance / Net                                Pin      Pin               Arrival     No. of    
Name                            Type          Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------------
internal_register_select[9]     DFFCE         Q        Out     0.243     0.243       -         
internal_register_select[9]     Net           -        -       0.535     -           1         
match_unit_rd_en_2_4[0]         LUT4          I1       In      -         0.778       -         
match_unit_rd_en_2_4[0]         LUT4          F        Out     0.570     1.348       -         
match_unit_rd_en_2_4[0]         Net           -        -       0.535     -           1         
match_unit_rd_en_2[0]           MUX2_LUT5     S0       In      -         1.883       -         
match_unit_rd_en_2[0]           MUX2_LUT5     O        Out     0.269     2.152       -         
internal_reg_start_m_14         Net           -        -       0.596     -           18        
data_from_internal_reg79        LUT3          I2       In      -         2.748       -         
data_from_internal_reg79        LUT3          F        Out     0.462     3.210       -         
data_from_internal_reg79        Net           -        -       0.596     -           16        
data_from_ao_reg_1[4]           LUT4          I1       In      -         3.806       -         
data_from_ao_reg_1[4]           LUT4          F        Out     0.570     4.376       -         
data_from_ao_reg_1[4]           Net           -        -       0.401     -           1         
data_from_ao_reg_2[4]           LUT4          I1       In      -         4.777       -         
data_from_ao_reg_2[4]           LUT4          F        Out     0.570     5.347       -         
data_from_ao_reg_2[4]           Net           -        -       0.401     -           1         
data_out_shift_reg_4_0[4]       LUT4          I0       In      -         5.748       -         
data_out_shift_reg_4_0[4]       LUT4          F        Out     0.549     6.297       -         
N_424                           Net           -        -       0.401     -           1         
data_out_shift_reg_4[4]         LUT3          I0       In      -         6.699       -         
data_out_shift_reg_4[4]         LUT3          F        Out     0.549     7.248       -         
data_out_shift_reg_4[4]         Net           -        -       0.000     -           1         
data_out_shift_reg[4]           DFFCE         D        In      -         7.248       -         
===============================================================================================
Total path delay (propagation time + setup) of 7.309 is 3.843(52.6%) logic and 3.466(47.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 2: 
      Requested Period:                      6.212
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         6.151

    - Propagation time:                      7.248
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (critical) :                     -1.096

    Number of logic level(s):                7
    Starting point:                          internal_register_select[9] / Q
    Ending point:                            data_out_shift_reg[3] / D
    The start point is clocked by            ao_top_0|control[0] [rising] on pin CLK
    The end   point is clocked by            ao_top_0|control[0] [rising] on pin CLK

Instance / Net                                Pin      Pin               Arrival     No. of    
Name                            Type          Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------------
internal_register_select[9]     DFFCE         Q        Out     0.243     0.243       -         
internal_register_select[9]     Net           -        -       0.535     -           1         
match_unit_rd_en_2_4[0]         LUT4          I1       In      -         0.778       -         
match_unit_rd_en_2_4[0]         LUT4          F        Out     0.570     1.348       -         
match_unit_rd_en_2_4[0]         Net           -        -       0.535     -           1         
match_unit_rd_en_2[0]           MUX2_LUT5     S0       In      -         1.883       -         
match_unit_rd_en_2[0]           MUX2_LUT5     O        Out     0.269     2.152       -         
internal_reg_start_m_14         Net           -        -       0.596     -           18        
data_from_internal_reg80        LUT3          I2       In      -         2.748       -         
data_from_internal_reg80        LUT3          F        Out     0.462     3.210       -         
data_from_internal_reg80        Net           -        -       0.596     -           16        
data_from_ao_reg_0[3]           LUT4          I1       In      -         3.806       -         
data_from_ao_reg_0[3]           LUT4          F        Out     0.570     4.376       -         
data_from_ao_reg_0[3]           Net           -        -       0.401     -           1         
data_from_ao_reg_4[3]           LUT4          I1       In      -         4.777       -         
data_from_ao_reg_4[3]           LUT4          F        Out     0.570     5.347       -         
data_from_ao_reg_4[3]           Net           -        -       0.401     -           1         
data_out_shift_reg_4_0[3]       LUT4          I0       In      -         5.748       -         
data_out_shift_reg_4_0[3]       LUT4          F        Out     0.549     6.297       -         
N_423                           Net           -        -       0.401     -           1         
data_out_shift_reg_4[3]         LUT3          I0       In      -         6.699       -         
data_out_shift_reg_4[3]         LUT3          F        Out     0.549     7.248       -         
data_out_shift_reg_4[3]         Net           -        -       0.000     -           1         
data_out_shift_reg[3]           DFFCE         D        In      -         7.248       -         
===============================================================================================
Total path delay (propagation time + setup) of 7.309 is 3.843(52.6%) logic and 3.466(47.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 3: 
      Requested Period:                      6.212
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         6.151

    - Propagation time:                      7.248
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (critical) :                     -1.096

    Number of logic level(s):                7
    Starting point:                          internal_register_select[9] / Q
    Ending point:                            data_out_shift_reg[6] / D
    The start point is clocked by            ao_top_0|control[0] [rising] on pin CLK
    The end   point is clocked by            ao_top_0|control[0] [rising] on pin CLK

Instance / Net                                Pin      Pin               Arrival     No. of    
Name                            Type          Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------------
internal_register_select[9]     DFFCE         Q        Out     0.243     0.243       -         
internal_register_select[9]     Net           -        -       0.535     -           1         
match_unit_rd_en_2_4[0]         LUT4          I1       In      -         0.778       -         
match_unit_rd_en_2_4[0]         LUT4          F        Out     0.570     1.348       -         
match_unit_rd_en_2_4[0]         Net           -        -       0.535     -           1         
match_unit_rd_en_2[0]           MUX2_LUT5     S0       In      -         1.883       -         
match_unit_rd_en_2[0]           MUX2_LUT5     O        Out     0.269     2.152       -         
internal_reg_start_m_14         Net           -        -       0.596     -           18        
data_from_internal_reg79        LUT3          I2       In      -         2.748       -         
data_from_internal_reg79        LUT3          F        Out     0.462     3.210       -         
data_from_internal_reg79        Net           -        -       0.596     -           16        
data_from_ao_reg_1[6]           LUT4          I1       In      -         3.806       -         
data_from_ao_reg_1[6]           LUT4          F        Out     0.570     4.376       -         
data_from_ao_reg_1[6]           Net           -        -       0.401     -           1         
data_from_ao_reg_2[6]           LUT4          I1       In      -         4.777       -         
data_from_ao_reg_2[6]           LUT4          F        Out     0.570     5.347       -         
data_from_ao_reg_2[6]           Net           -        -       0.401     -           1         
data_out_shift_reg_4_0[6]       LUT4          I0       In      -         5.748       -         
data_out_shift_reg_4_0[6]       LUT4          F        Out     0.549     6.297       -         
N_426                           Net           -        -       0.401     -           1         
data_out_shift_reg_4[6]         LUT3          I0       In      -         6.699       -         
data_out_shift_reg_4[6]         LUT3          F        Out     0.549     7.248       -         
data_out_shift_reg_4[6]         Net           -        -       0.000     -           1         
data_out_shift_reg[6]           DFFCE         D        In      -         7.248       -         
===============================================================================================
Total path delay (propagation time + setup) of 7.309 is 3.843(52.6%) logic and 3.466(47.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 4: 
      Requested Period:                      6.212
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         6.151

    - Propagation time:                      7.248
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (critical) :                     -1.096

    Number of logic level(s):                7
    Starting point:                          internal_register_select[9] / Q
    Ending point:                            data_out_shift_reg[7] / D
    The start point is clocked by            ao_top_0|control[0] [rising] on pin CLK
    The end   point is clocked by            ao_top_0|control[0] [rising] on pin CLK

Instance / Net                                Pin      Pin               Arrival     No. of    
Name                            Type          Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------------
internal_register_select[9]     DFFCE         Q        Out     0.243     0.243       -         
internal_register_select[9]     Net           -        -       0.535     -           1         
match_unit_rd_en_2_4[0]         LUT4          I1       In      -         0.778       -         
match_unit_rd_en_2_4[0]         LUT4          F        Out     0.570     1.348       -         
match_unit_rd_en_2_4[0]         Net           -        -       0.535     -           1         
match_unit_rd_en_2[0]           MUX2_LUT5     S0       In      -         1.883       -         
match_unit_rd_en_2[0]           MUX2_LUT5     O        Out     0.269     2.152       -         
internal_reg_start_m_14         Net           -        -       0.596     -           18        
data_from_internal_reg79        LUT3          I2       In      -         2.748       -         
data_from_internal_reg79        LUT3          F        Out     0.462     3.210       -         
data_from_internal_reg79        Net           -        -       0.596     -           16        
data_from_ao_reg_1[7]           LUT4          I1       In      -         3.806       -         
data_from_ao_reg_1[7]           LUT4          F        Out     0.570     4.376       -         
data_from_ao_reg_1[7]           Net           -        -       0.401     -           1         
data_from_ao_reg_2[7]           LUT4          I1       In      -         4.777       -         
data_from_ao_reg_2[7]           LUT4          F        Out     0.570     5.347       -         
data_from_ao_reg_2[7]           Net           -        -       0.401     -           1         
data_out_shift_reg_4_0[7]       LUT4          I0       In      -         5.748       -         
data_out_shift_reg_4_0[7]       LUT4          F        Out     0.549     6.297       -         
N_427                           Net           -        -       0.401     -           1         
data_out_shift_reg_4[7]         LUT3          I0       In      -         6.699       -         
data_out_shift_reg_4[7]         LUT3          F        Out     0.549     7.248       -         
data_out_shift_reg_4[7]         Net           -        -       0.000     -           1         
data_out_shift_reg[7]           DFFCE         D        In      -         7.248       -         
===============================================================================================
Total path delay (propagation time + setup) of 7.309 is 3.843(52.6%) logic and 3.466(47.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value


Path information for path number 5: 
      Requested Period:                      6.212
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         6.151

    - Propagation time:                      7.248
    - Clock delay at starting point:         0.000 (ideal)
    = Slack (critical) :                     -1.096

    Number of logic level(s):                7
    Starting point:                          internal_register_select[9] / Q
    Ending point:                            data_out_shift_reg[5] / D
    The start point is clocked by            ao_top_0|control[0] [rising] on pin CLK
    The end   point is clocked by            ao_top_0|control[0] [rising] on pin CLK

Instance / Net                                Pin      Pin               Arrival     No. of    
Name                            Type          Name     Dir     Delay     Time        Fan Out(s)
-----------------------------------------------------------------------------------------------
internal_register_select[9]     DFFCE         Q        Out     0.243     0.243       -         
internal_register_select[9]     Net           -        -       0.535     -           1         
match_unit_rd_en_2_4[0]         LUT4          I1       In      -         0.778       -         
match_unit_rd_en_2_4[0]         LUT4          F        Out     0.570     1.348       -         
match_unit_rd_en_2_4[0]         Net           -        -       0.535     -           1         
match_unit_rd_en_2[0]           MUX2_LUT5     S0       In      -         1.883       -         
match_unit_rd_en_2[0]           MUX2_LUT5     O        Out     0.269     2.152       -         
internal_reg_start_m_14         Net           -        -       0.596     -           18        
data_from_internal_reg79        LUT3          I2       In      -         2.748       -         
data_from_internal_reg79        LUT3          F        Out     0.462     3.210       -         
data_from_internal_reg79        Net           -        -       0.596     -           16        
data_from_ao_reg_1[5]           LUT4          I1       In      -         3.806       -         
data_from_ao_reg_1[5]           LUT4          F        Out     0.570     4.376       -         
data_from_ao_reg_1[5]           Net           -        -       0.401     -           1         
data_from_ao_reg_2[5]           LUT4          I1       In      -         4.777       -         
data_from_ao_reg_2[5]           LUT4          F        Out     0.570     5.347       -         
data_from_ao_reg_2[5]           Net           -        -       0.401     -           1         
data_out_shift_reg_4_0[5]       LUT4          I0       In      -         5.748       -         
data_out_shift_reg_4_0[5]       LUT4          F        Out     0.549     6.297       -         
N_425                           Net           -        -       0.401     -           1         
data_out_shift_reg_4[5]         LUT3          I0       In      -         6.699       -         
data_out_shift_reg_4[5]         LUT3          F        Out     0.549     7.248       -         
data_out_shift_reg_4[5]         Net           -        -       0.000     -           1         
data_out_shift_reg[5]           DFFCE         D        In      -         7.248       -         
===============================================================================================
Total path delay (propagation time + setup) of 7.309 is 3.843(52.6%) logic and 3.466(47.4%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value




====================================
Detailed Report for Clock: System
====================================



Starting Points with Worst Slack
********************************

                                         Starting                                           Arrival          
Instance                                 Reference     Type     Pin     Net                 Time        Slack
                                         Clock                                                               
-------------------------------------------------------------------------------------------------------------
u_ao_mem_ctrl.capture_mem_wr_RNIQKR6     System        INV      O       capture_end         0.000       2.284
address_counter_cry_0_RNO[0]             System        INV      O       address_counter     0.000       4.296
=============================================================================================================


Ending Points with Worst Slack
******************************

                              Starting                                                        Required          
Instance                      Reference     Type      Pin     Net                             Time         Slack
                              Clock                                                                             
----------------------------------------------------------------------------------------------------------------
capture_window_sel[2]         System        DFFC      D       capture_window_sel_3[2]         4.365        2.284
capture_window_sel[3]         System        DFFC      D       capture_window_sel_3[3]         4.365        2.284
capture_window_sel[1]         System        DFFC      D       capture_window_sel_3[1]         4.365        2.509
capture_window_sel[0]         System        DFFC      D       capture_window_sel_3[0]         4.365        3.281
internal_reg_start_dly[0]     System        DFFC      D       internal_reg_start_dly_2[0]     4.365        3.281
capture_end_dly               System        DFFP      D       capture_end                     4.365        3.830
address_counter[9]            System        DFFCE     D       address_counter_s[9]            6.151        4.296
address_counter[8]            System        DFFCE     D       address_counter_s[8]            6.151        4.331
address_counter[7]            System        DFFCE     D       address_counter_s[7]            6.151        4.366
address_counter[6]            System        DFFCE     D       address_counter_s[6]            6.151        4.401
================================================================================================================



Worst Path Information
***********************


Path information for path number 1: 
      Requested Period:                      4.426
    - Setup time:                            0.061
    + Clock delay at ending point:           0.000 (ideal)
    = Required time:                         4.365

    - Propagation time:                      2.081
    - Clock delay at starting point:         0.000 (ideal)
    - Estimated clock delay at start point:  -0.000
    = Slack (non-critical) :                 2.284

    Number of logic level(s):                2
    Starting point:                          u_ao_mem_ctrl.capture_mem_wr_RNIQKR6 / O
    Ending point:                            capture_window_sel[2] / D
    The start point is clocked by            System [rising]
    The end   point is clocked by            ao_top_0|clk_i [rising] on pin CLK

Instance / Net                                    Pin      Pin               Arrival     No. of    
Name                                     Type     Name     Dir     Delay     Time        Fan Out(s)
---------------------------------------------------------------------------------------------------
u_ao_mem_ctrl.capture_mem_wr_RNIQKR6     INV      O        Out     0.000     0.000       -         
capture_end                              Net      -        -       0.535     -           6         
un1_capture_window_sel_ac0_1             LUT4     I0       In      -         0.535       -         
un1_capture_window_sel_ac0_1             LUT4     F        Out     0.549     1.084       -         
un1_capture_window_sel_c2                Net      -        -       0.535     -           2         
capture_window_sel_3[2]                  LUT3     I2       In      -         1.619       -         
capture_window_sel_3[2]                  LUT3     F        Out     0.462     2.081       -         
capture_window_sel_3[2]                  Net      -        -       0.000     -           1         
capture_window_sel[2]                    DFFC     D        In      -         2.081       -         
===================================================================================================
Total path delay (propagation time + setup) of 2.142 is 1.072(50.0%) logic and 1.070(50.0%) route.
Path delay compensated for clock skew. Clock skew is added to clock-to-out value, and is subtracted from setup time value



##### END OF TIMING REPORT #####]

Timing exceptions that could not be applied
None

Finished final timing analysis (Real Time elapsed 0h:00m:06s; CPU Time elapsed 0h:00m:06s; Memory used current: 220MB peak: 223MB)


Finished timing report (Real Time elapsed 0h:00m:06s; CPU Time elapsed 0h:00m:06s; Memory used current: 220MB peak: 223MB)

---------------------------------------
Resource Usage Report for ao_top_0 

Mapping to part: gw2a_55pbga484-8
Cell usage:
ALU             85 uses
DFF             16 uses
DFFC            44 uses
DFFCE           207 uses
DFFNP           2 uses
DFFP            3 uses
DFFPE           32 uses
GSR             1 use
INV             2 uses
MUX2_LUT5       8 uses
MUX2_LUT6       3 uses
SDPX9           1 use
LUT2            48 uses
LUT3            111 uses
LUT4            270 uses

I/O ports: 35
I/O primitives: 35
IBUF           33 uses
OBUF           2 uses

I/O Register bits:                  0
Register bits not including I/Os:   304 of 41040 (0%)

RAM/ROM usage summary
Block Rams : 1 of 140 (0%)

Total load per clock:
   ao_top_0|clk_i: 1
   ao_top_0|control[0]: 247

@S |Mapping Summary:
Total  LUTs: 429 (0%)

Mapper successful!

At Mapper Exit (Real Time elapsed 0h:00m:07s; CPU Time elapsed 0h:00m:06s; Memory used current: 45MB peak: 223MB)

Process took 0h:00m:07s realtime, 0h:00m:06s cputime
# Wed Sep 19 08:40:01 2018

###########################################################]
