@P:  Worst Slack : -0.485
@P:  RAM_based_shift_reg_top|clk - Estimated Frequency : 309.2 MHz
@P:  RAM_based_shift_reg_top|clk - Requested Frequency : 363.8 MHz
@P:  RAM_based_shift_reg_top|clk - Estimated Period : 3.234
@P:  RAM_based_shift_reg_top|clk - Requested Period : 2.749
@P:  RAM_based_shift_reg_top|clk - Slack : -0.485
@P: RAM_based_shift_reg_top Part : gw2a_55pbga484-8
@P: RAM_based_shift_reg_top I/O Register bits : 0
@P: RAM_based_shift_reg_top Register bits (Non I/O) : 9 (0%)
@P: RAM_based_shift_reg_top Block Rams : 1 of 140 (0%)
@P: RAM_based_shift_reg_top Total Luts : 20 of 800 (0%)
@P:  CPU Time : 0h:00m:02s
