//Copyright (C)2014-2020 Gowin Semiconductor Corporation.
//All rights reserved.


1. PnR Messages

  <Report Title>: Gowin PnR Report
  <Design File>: E:\IP_verify\1.9.6\IP_web\Gowin_Scaler_RefDesign_DDR300MHz\Gowin_Scaler_RefDesign_DDR300MHz\scaler_example_design_live\project\impl\synthesize\rev_1\scaler_ref_design_live.vm
  <Physical Constraints File>: E:\IP_verify\1.9.6\IP_web\Gowin_Scaler_RefDesign_DDR300MHz\Gowin_Scaler_RefDesign_DDR300MHz\scaler_example_design_live\project\src\scaler_test_top.cst
  <Timing Constraints File>: E:\IP_verify\1.9.6\IP_web\Gowin_Scaler_RefDesign_DDR300MHz\Gowin_Scaler_RefDesign_DDR300MHz\scaler_example_design_live\project\src\scaler_ref_design_live.sdc
  <GOWIN Version>: V1.9.6Beta
  <Part Number>: GW2A-LV18PG484C8/I7
  <Created Time>:Wed Jul 01 18:05:55 2020


2. Placer

  Starting Placer:
    Placement Phase 0 ...   REAL time: 2.536 secs
    Placement Phase 1 ...   REAL time: 0.497 secs
    Placement Phase 2 ...   REAL time: 3.79 secs
    Placement Phase 3 ...   REAL time: 42.088 secs
  Total REAL time to Placement completion: 48.911 secs.


3. Resource Usage Summary

  ----------------------------------------------------------
  Resources            | Usage
  ----------------------------------------------------------
  Logic                | 5663/20736  27%
    --LUT,ALU,ROM16    | 5195(4112 LUT, 1083 ALU, 0 ROM16)
    --SSRAM(RAM16)     | 78
  Register             | 4043/16512  24%
    --Logic Register   | 4023/15552  25%
    --I/O Register     | 20/960  2%
  CLS                  | 3719/10368  35%
  I/O Port             | 83
  I/O Buf              | 80
    --Input Buf        | 2
    --Output Buf       | 58
    --Inout Buf        | 20
  IOLOGIC              | 36%
    --IDES8_MEM        | 16
    --OSER8            | 23
    --OSER8_MEM        | 20
    --IODELAY          | 16
  BSRAM                | 73%
    --SDP              | 9
    --SDPX9            | 7
    --SDPB             | 18
  DSP                  | 25%
    --MULT18X18        | 12
  PLL                  | 3/4  75%
  DCS                  | 0/8  0%
  DQCE                 | 0/24  0%
  OSC                  | 0/1  0%
  CLKDIV               | 1/8  12%
  DLLDLY               | 0/8  0%
  DQS                  | 2/16  12%
  DHCEN                | 1/16  6%
  ==========================================================



4. I/O Bank Usage Summary

  -----------------------
  I/O Bank  | Usage       
  -----------------------
  bank 0   | 0/40(0%)    
  bank 1   | 2/40(5%)    
  bank 2   | 30/46(65%)  
  bank 3   | 8/34(23%)   
  bank 4   | 0/40(0%)    
  bank 5   | 0/40(0%)    
  bank 6   | 17/34(50%)  
  bank 7   | 23/46(50%)  
  =======================


5. Router

  Starting Router:
    Route Phase 0: 13425 unrouted; REAL time: 0.003 secs
    Route Phase 1: 8058 unrouted; REAL time: 0.913 secs
    Route Phase 2: 0  unrouted; REAL time: 6.334 secs
  Total REAL time to Router completion: 7.25 secs.


6. Global Clock Usage Summary

  -------------------------------
  Global Clock  | Usage       
  -------------------------------
  PRIMARY       | 5/8(62%)
  SECONDARY     | 8/8(100%)
  GCLK_PIN      | 2/8(25%)
  PLL           | 3/4(75%)
  CLKDIV        | 1/8(12%)
  DLLDLY        | 0/8(0%)
  ===============================


7. Global Clock Signals

  -------------------------------------------
  Signal         | Global Clock   | Location
  -------------------------------------------
  clkout         | PRIMARY        |  TR TL BR BL
  dma_clk        | PRIMARY        |  TR TL BR BL
  I_clk_c        | PRIMARY        |  TR TL BR BL
  O_adv7513_clk_c| PRIMARY        |  TR
  D0_L3          | PRIMARY        |  TL BL
  rst_n1         | SECONDARY      |  -
  init_calib_complete| SECONDARY      |  -
  I_rst_n_c_i    | SECONDARY      |  -
  rst_n1_i       | SECONDARY      |  -
  frame_rst      | SECONDARY      |  -
  un1_vval_limit_en_1_i_sx_RNII8VE| SECONDARY      |  -
  ddr_rstz       | SECONDARY      |  -
  raddr_dly3     | SECONDARY      |  -
  clk_x4         | HCLK           | LEFT[0] RIGHT[0]
  ===========================================


8. Pinout by Port Name

----------------------------------------------------------------------------------------------------------------------------------------------------------
Port Name           | Loc./Bank  | Dir.  | Site     | IO Type    | Drive      | Pull Mode  | Slew Rate  | PCI Clamp  | OpenDrain  | VREF       | BankVccio 
----------------------------------------------------------------------------------------------------------------------------------------------------------
I_clk               | M19/2      | in    | IOR27[A] | LVCMOS33   | NA         | UP         | NA         | NA         | NA         | NA         | 3.3       
I_rst_n             | L22/2      | in    | IOR21[B] | LVCMOS33   | NA         | UP         | NA         | NA         | NA         | NA         | 3.3       
O_led[0]            | W20/3      | out   | IOR48[A] | LVCMOS15   | 8          | UP         | FAST       | NA         | OFF        | NA         | 1.5       
O_led[1]            | W22/3      | out   | IOR36[B] | LVCMOS15   | 8          | UP         | FAST       | NA         | OFF        | NA         | 1.5       
O_led[2]            | V22/3      | out   | IOR36[A] | LVCMOS15   | 8          | UP         | FAST       | NA         | OFF        | NA         | 1.5       
O_led[3]            | U20/3      | out   | IOR38[B] | LVCMOS15   | 8          | UP         | FAST       | NA         | OFF        | NA         | 1.5       
O_adv7513_clk       | H21/2      | out   | IOR15[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_vs        | L19/2      | out   | IOR22[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_hs        | K22/2      | out   | IOR21[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_de        | K20/2      | out   | IOR23[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[0]   | K18/2      | out   | IOR9[B]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[1]   | K19/2      | out   | IOR22[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[2]   | J22/2      | out   | IOR20[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[3]   | J19/2      | out   | IOR16[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[4]   | J18/2      | out   | IOR9[A]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[5]   | J20/2      | out   | IOR16[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[6]   | H22/2      | out   | IOR20[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[7]   | H19/2      | out   | IOR5[A]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[8]   | H18/2      | out   | IOR5[B]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[9]   | H20/2      | out   | IOR15[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[10]  | G18/2      | out   | IOR4[B]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[11]  | G19/2      | out   | IOR11[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[12]  | G20/2      | out   | IOR11[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[13]  | G22/2      | out   | IOR18[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[14]  | F18/2      | out   | IOR2[A]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[15]  | G21/2      | out   | IOR18[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[16]  | F19/2      | out   | IOR2[B]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[17]  | F20/2      | out   | IOR12[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[18]  | F22/2      | out   | IOR17[A] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[19]  | F21/2      | out   | IOR12[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[20]  | E20/2      | out   | IOR3[B]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[21]  | E22/2      | out   | IOR17[B] | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[22]  | E19/2      | out   | IOR3[A]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_adv7513_data[23]  | D20/2      | out   | IOR6[B]  | LVCMOS33   | 8          | UP         | FAST       | NA         | OFF        | NA         | 3.3       
O_ddr_addr[0]       | G1/7       | out   | IOL15[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[1]       | U5/6       | out   | IOL53[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[2]       | G5/7       | out   | IOL4[B]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[3]       | F5/7       | out   | IOL2[B]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[4]       | V3/6       | out   | IOL44[A] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[5]       | G2/7       | out   | IOL14[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[6]       | AA22/3     | out   | IOR44[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[7]       | H5/7       | out   | IOL9[A]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[8]       | AB22/3     | out   | IOR50[A] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[9]       | J4/7       | out   | IOL16[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[10]      | R5/6       | out   | IOL47[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[11]      | AA21/3     | out   | IOR47[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[12]      | T5/6       | out   | IOL54[A] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_addr[13]      | AA1/6      | out   | IOL45[A] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_ba[0]         | F4/7       | out   | IOL7[A]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_ba[1]         | U4/6       | out   | IOL48[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_ba[2]         | F3/7       | out   | IOL8[A]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_ras_n         | D1/7       | out   | IOL12[A] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_cas_n         | C3/7       | out   | IOL5[B]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_we_n          | C1/7       | out   | IOL11[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_clk           | P22/3      | out   | IOR29[A] | SSTL15D    | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_clk_n         | R22/3      | out   | IOR29[B] | SSTL15D    | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_cke           | E3/7       | out   | IOL6[B]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_odt           | B2/7       | out   | IOL3[B]  | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_reset_n       | W4/6       | out   | IOL50[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_dqm[0]        | R3/6       | out   | IOL35[B] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
O_ddr_dqm[1]        | K4/7       | out   | IOL24[A] | SSTL15     | 8          | NA         | FAST       | NA         | NA         | NA         | 1.5       
IO_adv7513_scl      | A20/1      | io    | IOT43[A] | LVCMOS25   | 8          | UP         | FAST       | NA         | OFF        | NA         | 2.5       
IO_adv7513_sda      | A21/1      | io    | IOT43[B] | LVCMOS25   | 8          | UP         | FAST       | NA         | OFF        | NA         | 2.5       
IO_ddr_dq[0]        | M5/6       | io    | IOL32[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[1]        | T3/6       | io    | IOL39[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[2]        | M3/6       | io    | IOL29[B] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[3]        | T2/6       | io    | IOL33[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[4]        | Y1/6       | io    | IOL38[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[5]        | U1/6       | io    | IOL30[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[6]        | N3/6       | io    | IOL31[B] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[7]        | V1/6       | io    | IOL34[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[8]        | T1/7       | io    | IOL27[B] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[9]        | K3/7       | io    | IOL23[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[10]       | P1/7       | io    | IOL26[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[11]       | J1/7       | io    | IOL20[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[12]       | L5/7       | io    | IOL21[B] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[13]       | H3/7       | io    | IOL17[A] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[14]       | M1/7       | io    | IOL25[B] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dq[15]       | H1/7       | io    | IOL18[B] | SSTL15     | 8          | UP         | FAST       | NA         | NA         | INTERNAL   | 1.5       
IO_ddr_dqs[0]       | P4/6       | io    | IOL36[A] | SSTL15D    | 8          | UP         | FAST       | NA         | NA         | NA         | 1.5       
IO_ddr_dqs[1]       | L2/7       | io    | IOL22[A] | SSTL15D    | 8          | UP         | FAST       | NA         | NA         | NA         | 1.5       
IO_ddr_dqs_n[0]     | R4/6       | io    | IOL36[B] | SSTL15D    | 8          | UP         | FAST       | NA         | NA         | NA         | 1.5       
IO_ddr_dqs_n[1]     | L1/7       | io    | IOL22[B] | SSTL15D    | 8          | UP         | FAST       | NA         | NA         | NA         | 1.5       
==========================================================================================================================================================




9. All Package Pins

----------------------------------------------------------------------------------------------------------------------------------
Loc./Bank| Signal              | Dir.  | Site     | IO Type  | Pull Mode | OpenDrain | Hysteresis | DiffResistor | SingleResistor
----------------------------------------------------------------------------------------------------------------------------------
D5/0     | UNUSED              | in    | IOT2[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D6/0     | UNUSED              | in    | IOT2[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E6/0     | UNUSED              | in    | IOT3[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E7/0     | UNUSED              | in    | IOT3[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D4/0     | UNUSED              | in    | IOT4[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C4/0     | UNUSED              | in    | IOT4[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
F6/0     | UNUSED              | in    | IOT6[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
F7/0     | UNUSED              | in    | IOT6[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C5/0     | UNUSED              | in    | IOT7[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C6/0     | UNUSED              | in    | IOT7[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B1/0     | UNUSED              | in    | IOT9[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A1/0     | UNUSED              | in    | IOT9[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D7/0     | UNUSED              | in    | IOT13[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D8/0     | UNUSED              | in    | IOT13[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A2/0     | UNUSED              | in    | IOT14[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A3/0     | UNUSED              | in    | IOT14[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C7/0     | UNUSED              | in    | IOT16[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C8/0     | UNUSED              | in    | IOT16[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A4/0     | UNUSED              | in    | IOT17[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A5/0     | UNUSED              | in    | IOT17[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B6/0     | UNUSED              | in    | IOT18[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A6/0     | UNUSED              | in    | IOT18[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E8/0     | UNUSED              | in    | IOT19[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E9/0     | UNUSED              | in    | IOT19[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D9/0     | UNUSED              | in    | IOT20[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D10/0    | UNUSED              | in    | IOT20[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B7/0     | UNUSED              | in    | IOT21[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A7/0     | UNUSED              | in    | IOT21[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C9/0     | UNUSED              | in    | IOT22[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C10/0    | UNUSED              | in    | IOT22[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B8/0     | UNUSED              | in    | IOT23[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A8/0     | UNUSED              | in    | IOT23[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A9/0     | UNUSED              | in    | IOT24[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A10/0    | UNUSED              | in    | IOT24[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E10/0    | UNUSED              | in    | IOT25[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E11/0    | UNUSED              | in    | IOT25[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A11/0    | UNUSED              | in    | IOT26[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A12/0    | UNUSED              | in    | IOT26[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B11/0    | UNUSED              | in    | IOT27[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B12/0    | UNUSED              | in    | IOT27[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D11/1    | UNUSED              | in    | IOT30[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D12/1    | UNUSED              | in    | IOT30[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C11/1    | UNUSED              | in    | IOT31[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C12/1    | UNUSED              | in    | IOT31[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E12/1    | UNUSED              | in    | IOT32[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E13/1    | UNUSED              | in    | IOT32[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A13/1    | UNUSED              | in    | IOT33[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A14/1    | UNUSED              | in    | IOT33[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A15/1    | UNUSED              | in    | IOT34[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B15/1    | UNUSED              | in    | IOT34[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C13/1    | UNUSED              | in    | IOT35[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D13/1    | UNUSED              | in    | IOT35[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C14/1    | UNUSED              | in    | IOT36[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C15/1    | UNUSED              | in    | IOT36[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A16/1    | UNUSED              | in    | IOT37[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B16/1    | UNUSED              | in    | IOT37[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A17/1    | UNUSED              | in    | IOT38[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B17/1    | UNUSED              | in    | IOT38[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D14/1    | UNUSED              | in    | IOT39[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D15/1    | UNUSED              | in    | IOT39[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A18/1    | UNUSED              | in    | IOT40[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A19/1    | UNUSED              | in    | IOT40[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C16/1    | UNUSED              | in    | IOT41[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C17/1    | UNUSED              | in    | IOT41[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A20/1    | IO_adv7513_scl      | io    | IOT43[A] | LVCMOS25 | UP        | OFF       | NONE       | NA           | NA            
A21/1    | IO_adv7513_sda      | io    | IOT43[B] | LVCMOS25 | UP        | OFF       | NONE       | NA           | NA            
C18/1    | UNUSED              | in    | IOT44[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C19/1    | UNUSED              | in    | IOT44[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D16/1    | UNUSED              | in    | IOT48[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E16/1    | UNUSED              | in    | IOT48[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E14/1    | UNUSED              | in    | IOT50[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E15/1    | UNUSED              | in    | IOT50[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D17/1    | UNUSED              | in    | IOT51[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D18/1    | UNUSED              | in    | IOT51[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
F16/1    | UNUSED              | in    | IOT53[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
F17/1    | UNUSED              | in    | IOT53[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
A22/1    | UNUSED              | in    | IOT54[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B22/1    | UNUSED              | in    | IOT54[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E17/1    | UNUSED              | in    | IOT55[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E18/1    | UNUSED              | in    | IOT55[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
----------------------------------------------------------------------------------------------------------------------------------
U6/5     | UNUSED              | in    | IOB2[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U7/5     | UNUSED              | in    | IOB2[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W5/5     | UNUSED              | in    | IOB3[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W6/5     | UNUSED              | in    | IOB3[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V6/5     | UNUSED              | in    | IOB4[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V7/5     | UNUSED              | in    | IOB4[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y4/5     | UNUSED              | in    | IOB6[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y5/5     | UNUSED              | in    | IOB6[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V8/5     | UNUSED              | in    | IOB7[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V9/5     | UNUSED              | in    | IOB7[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y3/5     | UNUSED              | in    | IOB9[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA3/5    | UNUSED              | in    | IOB9[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB1/5    | UNUSED              | in    | IOB13[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB2/5    | UNUSED              | in    | IOB13[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y6/5     | UNUSED              | in    | IOB14[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA6/5    | UNUSED              | in    | IOB14[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W7/5     | UNUSED              | in    | IOB16[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W8/5     | UNUSED              | in    | IOB16[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB3/5    | UNUSED              | in    | IOB17[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB4/5    | UNUSED              | in    | IOB17[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y7/5     | UNUSED              | in    | IOB18[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y8/5     | UNUSED              | in    | IOB18[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V10/5    | UNUSED              | in    | IOB19[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V11/5    | UNUSED              | in    | IOB19[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W9/5     | UNUSED              | in    | IOB20[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y9/5     | UNUSED              | in    | IOB20[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB5/5    | UNUSED              | in    | IOB21[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB6/5    | UNUSED              | in    | IOB21[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA7/5    | UNUSED              | in    | IOB22[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB7/5    | UNUSED              | in    | IOB22[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA8/5    | UNUSED              | in    | IOB23[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB8/5    | UNUSED              | in    | IOB23[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W10/5    | UNUSED              | in    | IOB24[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W11/5    | UNUSED              | in    | IOB24[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA11/5   | UNUSED              | in    | IOB25[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB11/5   | UNUSED              | in    | IOB25[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y10/5    | UNUSED              | in    | IOB26[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y11/5    | UNUSED              | in    | IOB26[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB9/5    | UNUSED              | in    | IOB27[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB10/5   | UNUSED              | in    | IOB27[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB12/4   | UNUSED              | in    | IOB30[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA12/4   | UNUSED              | in    | IOB30[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y12/4    | UNUSED              | in    | IOB31[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y13/4    | UNUSED              | in    | IOB31[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W12/4    | UNUSED              | in    | IOB32[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W13/4    | UNUSED              | in    | IOB32[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB13/4   | UNUSED              | in    | IOB33[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB14/4   | UNUSED              | in    | IOB33[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB15/4   | UNUSED              | in    | IOB34[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA15/4   | UNUSED              | in    | IOB34[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V12/4    | UNUSED              | in    | IOB35[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V13/4    | UNUSED              | in    | IOB35[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB16/4   | UNUSED              | in    | IOB36[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA16/4   | UNUSED              | in    | IOB36[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y14/4    | UNUSED              | in    | IOB37[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y15/4    | UNUSED              | in    | IOB37[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V14/4    | UNUSED              | in    | IOB38[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V15/4    | UNUSED              | in    | IOB38[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB17/4   | UNUSED              | in    | IOB39[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB18/4   | UNUSED              | in    | IOB39[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA17/4   | UNUSED              | in    | IOB40[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y17/4    | UNUSED              | in    | IOB40[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W14/4    | UNUSED              | in    | IOB41[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W15/4    | UNUSED              | in    | IOB41[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB19/4   | UNUSED              | in    | IOB43[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB20/4   | UNUSED              | in    | IOB43[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y16/4    | UNUSED              | in    | IOB44[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W16/4    | UNUSED              | in    | IOB44[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y19/4    | UNUSED              | in    | IOB48[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y18/4    | UNUSED              | in    | IOB48[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V16/4    | UNUSED              | in    | IOB50[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U16/4    | UNUSED              | in    | IOB50[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W17/4    | UNUSED              | in    | IOB51[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W18/4    | UNUSED              | in    | IOB51[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA20/4   | UNUSED              | in    | IOB53[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y20/4    | UNUSED              | in    | IOB53[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V17/4    | UNUSED              | in    | IOB54[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V18/4    | UNUSED              | in    | IOB54[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W19/4    | UNUSED              | in    | IOB55[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V19/4    | UNUSED              | in    | IOB55[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
----------------------------------------------------------------------------------------------------------------------------------
E5/7     | UNUSED              | in    | IOL2[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
F5/7     | O_ddr_addr[3]       | out   | IOL2[B]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
B3/7     | UNUSED              | in    | IOL3[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B2/7     | O_ddr_odt           | out   | IOL3[B]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
G6/7     | UNUSED              | in    | IOL4[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
G5/7     | O_ddr_addr[2]       | out   | IOL4[B]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
D3/7     | UNUSED              | in    | IOL5[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C3/7     | O_ddr_cas_n         | out   | IOL5[B]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
E4/7     | UNUSED              | in    | IOL6[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
E3/7     | O_ddr_cke           | out   | IOL6[B]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
F4/7     | O_ddr_ba[0]         | out   | IOL7[A]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
G4/7     | UNUSED              | in    | IOL7[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
F3/7     | O_ddr_ba[2]         | out   | IOL8[A]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
G3/7     | UNUSED              | in    | IOL8[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
H5/7     | O_ddr_addr[7]       | out   | IOL9[A]  | SSTL15   | NA        | NA        | NA         | NA           | OFF           
J5/7     | UNUSED              | in    | IOL9[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C2/7     | UNUSED              | in    | IOL11[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C1/7     | O_ddr_we_n          | out   | IOL11[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
D1/7     | O_ddr_ras_n         | out   | IOL12[A] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
E1/7     | UNUSED              | in    | IOL12[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
F2/7     | UNUSED              | in    | IOL14[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
G2/7     | O_ddr_addr[5]       | out   | IOL14[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
F1/7     | UNUSED              | in    | IOL15[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
G1/7     | O_ddr_addr[0]       | out   | IOL15[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
H4/7     | UNUSED              | in    | IOL16[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
J4/7     | O_ddr_addr[9]       | out   | IOL16[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
H3/7     | IO_ddr_dq[13]       | io    | IOL17[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
J3/7     | UNUSED              | in    | IOL17[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
H2/7     | UNUSED              | in    | IOL18[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
H1/7     | IO_ddr_dq[15]       | io    | IOL18[B] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
J1/7     | IO_ddr_dq[11]       | io    | IOL20[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
K1/7     | UNUSED              | in    | IOL20[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
K5/7     | UNUSED              | in    | IOL21[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
L5/7     | IO_ddr_dq[12]       | io    | IOL21[B] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
L2/7     | IO_ddr_dqs[1]       | io    | IOL22[A] | SSTL15D  | UP        | NA        | NA         | NA           | OFF           
L1/7     | IO_ddr_dqs_n[1]     | io    | IOL22[B] | SSTL15D  | UP        | NA        | NA         | NA           | OFF           
K3/7     | IO_ddr_dq[9]        | io    | IOL23[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
L3/7     | UNUSED              | in    | IOL23[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
K4/7     | O_ddr_dqm[1]        | out   | IOL24[A] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
L4/7     | UNUSED              | in    | IOL24[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M2/7     | UNUSED              | in    | IOL25[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M1/7     | IO_ddr_dq[14]       | io    | IOL25[B] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
P1/7     | IO_ddr_dq[10]       | io    | IOL26[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
N1/7     | UNUSED              | in    | IOL26[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
R1/7     | UNUSED              | in    | IOL27[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
T1/7     | IO_ddr_dq[8]        | io    | IOL27[B] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
M4/6     | UNUSED              | in    | IOL29[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M3/6     | IO_ddr_dq[2]        | io    | IOL29[B] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
U1/6     | IO_ddr_dq[5]        | io    | IOL30[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
U2/6     | UNUSED              | in    | IOL30[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
N4/6     | UNUSED              | in    | IOL31[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
N3/6     | IO_ddr_dq[6]        | io    | IOL31[B] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
M5/6     | IO_ddr_dq[0]        | io    | IOL32[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
N5/6     | UNUSED              | in    | IOL32[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
T2/6     | IO_ddr_dq[3]        | io    | IOL33[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
R2/6     | UNUSED              | in    | IOL33[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V1/6     | IO_ddr_dq[7]        | io    | IOL34[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
W1/6     | UNUSED              | in    | IOL34[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
P3/6     | UNUSED              | in    | IOL35[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
R3/6     | O_ddr_dqm[0]        | out   | IOL35[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
P4/6     | IO_ddr_dqs[0]       | io    | IOL36[A] | SSTL15D  | UP        | NA        | NA         | NA           | OFF           
R4/6     | IO_ddr_dqs_n[0]     | io    | IOL36[B] | SSTL15D  | UP        | NA        | NA         | NA           | OFF           
Y1/6     | IO_ddr_dq[4]        | io    | IOL38[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
Y2/6     | UNUSED              | in    | IOL38[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
T3/6     | IO_ddr_dq[1]        | io    | IOL39[A] | SSTL15   | UP        | NA        | NA         | NA           | OFF           
U3/6     | UNUSED              | in    | IOL39[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V3/6     | O_ddr_addr[4]       | out   | IOL44[A] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
W3/6     | UNUSED              | in    | IOL44[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA1/6    | O_ddr_addr[13]      | out   | IOL45[A] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
AA2/6    | UNUSED              | in    | IOL45[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
P5/6     | UNUSED              | in    | IOL47[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
R5/6     | O_ddr_addr[10]      | out   | IOL47[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
T4/6     | UNUSED              | in    | IOL48[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U4/6     | O_ddr_ba[1]         | out   | IOL48[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
V4/6     | UNUSED              | in    | IOL50[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
W4/6     | O_ddr_reset_n       | out   | IOL50[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
V5/6     | UNUSED              | in    | IOL53[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U5/6     | O_ddr_addr[1]       | out   | IOL53[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
T5/6     | O_ddr_addr[12]      | out   | IOL54[A] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
T6/6     | UNUSED              | in    | IOL54[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
----------------------------------------------------------------------------------------------------------------------------------
F18/2    | O_adv7513_data[14]  | out   | IOR2[A]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
F19/2    | O_adv7513_data[16]  | out   | IOR2[B]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
E19/2    | O_adv7513_data[22]  | out   | IOR3[A]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
E20/2    | O_adv7513_data[20]  | out   | IOR3[B]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
G17/2    | UNUSED              | in    | IOR4[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
G18/2    | O_adv7513_data[10]  | out   | IOR4[B]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
H19/2    | O_adv7513_data[7]   | out   | IOR5[A]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
H18/2    | O_adv7513_data[8]   | out   | IOR5[B]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
D19/2    | UNUSED              | in    | IOR6[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D20/2    | O_adv7513_data[23]  | out   | IOR6[B]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
B20/2    | UNUSED              | in    | IOR7[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C20/2    | UNUSED              | in    | IOR7[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
B21/2    | UNUSED              | in    | IOR8[A]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
C21/2    | UNUSED              | in    | IOR8[B]  | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
J18/2    | O_adv7513_data[4]   | out   | IOR9[A]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
K18/2    | O_adv7513_data[0]   | out   | IOR9[B]  | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
G19/2    | O_adv7513_data[11]  | out   | IOR11[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
G20/2    | O_adv7513_data[12]  | out   | IOR11[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
F20/2    | O_adv7513_data[17]  | out   | IOR12[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
F21/2    | O_adv7513_data[19]  | out   | IOR12[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
C22/2    | UNUSED              | in    | IOR14[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
D22/2    | UNUSED              | in    | IOR14[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
H20/2    | O_adv7513_data[9]   | out   | IOR15[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
H21/2    | O_adv7513_clk       | out   | IOR15[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
J19/2    | O_adv7513_data[3]   | out   | IOR16[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
J20/2    | O_adv7513_data[5]   | out   | IOR16[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
F22/2    | O_adv7513_data[18]  | out   | IOR17[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
E22/2    | O_adv7513_data[21]  | out   | IOR17[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
G21/2    | O_adv7513_data[15]  | out   | IOR18[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
G22/2    | O_adv7513_data[13]  | out   | IOR18[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
H22/2    | O_adv7513_data[6]   | out   | IOR20[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
J22/2    | O_adv7513_data[2]   | out   | IOR20[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
K22/2    | O_adv7513_hs        | out   | IOR21[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
L22/2    | I_rst_n             | in    | IOR21[B] | LVCMOS33 | UP        | NA        | NONE       | NA           | OFF           
K19/2    | O_adv7513_data[1]   | out   | IOR22[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
L19/2    | O_adv7513_vs        | out   | IOR22[B] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
K20/2    | O_adv7513_de        | out   | IOR23[A] | LVCMOS33 | UP        | OFF       | NA         | NA           | OFF           
L20/2    | UNUSED              | in    | IOR23[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
L21/2    | UNUSED              | in    | IOR24[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M21/2    | UNUSED              | in    | IOR24[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M22/2    | UNUSED              | out   | IOR25[A] | LVCMOS18 | UP        | OFF       | NA         | NA           | NA            
N22/2    | UNUSED              | in    | IOR25[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
N20/2    | UNUSED              | in    | IOR26[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M20/2    | UNUSED              | in    | IOR26[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M19/2    | I_clk               | in    | IOR27[A] | LVCMOS33 | UP        | NA        | NONE       | NA           | OFF           
N19/2    | UNUSED              | in    | IOR27[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
P22/3    | O_ddr_clk           | out   | IOR29[A] | SSTL15D  | NA        | NA        | NA         | NA           | OFF           
R22/3    | O_ddr_clk_n         | out   | IOR29[B] | SSTL15D  | NA        | NA        | NA         | NA           | OFF           
T22/3    | UNUSED              | in    | IOR30[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U22/3    | UNUSED              | in    | IOR30[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U21/3    | UNUSED              | in    | IOR31[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
T21/3    | UNUSED              | in    | IOR31[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
L18/3    | UNUSED              | in    | IOR32[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
M18/3    | UNUSED              | in    | IOR32[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
P19/3    | UNUSED              | in    | IOR33[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
P20/3    | UNUSED              | in    | IOR33[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
N18/3    | UNUSED              | in    | IOR34[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
P18/3    | UNUSED              | in    | IOR34[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
R20/3    | UNUSED              | in    | IOR35[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
R21/3    | UNUSED              | in    | IOR35[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
V22/3    | O_led[2]            | out   | IOR36[A] | LVCMOS15 | UP        | OFF       | NA         | NA           | OFF           
W22/3    | O_led[1]            | out   | IOR36[B] | LVCMOS15 | UP        | OFF       | NA         | NA           | OFF           
T20/3    | UNUSED              | in    | IOR38[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U20/3    | O_led[3]            | out   | IOR38[B] | LVCMOS15 | UP        | OFF       | NA         | NA           | OFF           
T19/3    | UNUSED              | in    | IOR39[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
R19/3    | UNUSED              | in    | IOR39[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y22/3    | UNUSED              | in    | IOR44[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA22/3   | O_ddr_addr[6]       | out   | IOR44[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
R18/3    | UNUSED              | in    | IOR45[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
T18/3    | UNUSED              | in    | IOR45[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
Y21/3    | UNUSED              | in    | IOR47[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AA21/3   | O_ddr_addr[11]      | out   | IOR47[B] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
W20/3    | O_led[0]            | out   | IOR48[A] | LVCMOS15 | UP        | OFF       | NA         | NA           | OFF           
V20/3    | UNUSED              | in    | IOR48[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
AB22/3   | O_ddr_addr[8]       | out   | IOR50[A] | SSTL15   | NA        | NA        | NA         | NA           | OFF           
AB21/3   | UNUSED              | in    | IOR50[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
T17/3    | UNUSED              | in    | IOR53[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U17/3    | UNUSED              | in    | IOR53[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U19/3    | UNUSED              | in    | IOR54[A] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
U18/3    | UNUSED              | in    | IOR54[B] | LVCMOS18 | UP        | NA        | NONE       | NA           | NA            
----------------------------------------------------------------------------------------------------------------------------------
==================================================================================================================================



  Placement and routing completed.


10. Memory usage: 290MB.
