Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | F:/user-bak/Users/FDELL/Desktop/IP/CrossCrorelation/Gowin_XCORR_RefDesign/XCORR_512-3_case/project/impl/synplify/rev_1/XCORR_512-3_case.vm
Physical Constraints File | F:\user-bak\Users\FDELL\Desktop\IP\CrossCrorelation\Gowin_XCORR_RefDesign\XCORR_512-3_case\project\src\XCORR_512-3_case.cst
Timing Constraints File | ---
GOWIN Version | v1.9.0Beta
Part Number | GW2A-LV55PG484C8/I7
Created Time | Tue Feb 19 17:22:56 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 240.410
Quiescent Power (mW) | 42.107
Dynamic Power (mW) | 198.302

## Thermal Information:

Junction Temperature | 37.584
Theta JA | 53.325
Max Allowed Ambient Temperature | 72.180

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_100
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 147.555 | 21.861 | 203.300
VCCX | 2.500 | 4.941 | 3.692 | 21.583
VCCO18 | 1.800 | 4.936 | 3.690 | 15.527

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 15.928 | NA | 12.500
IO | 47.470 | 20.304 | 13.580
Bsram | 79.294 | NA | NA

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
top | 113.135 | 37.323(34.724) | 75.812(67.943)
top/ut/ | 0.564 | 0.121(0.000) | 0.443(0.000)
top/uut/ | 102.103 | 34.603(34.603) | 67.500(67.500)
top/uut/u_xcorr/ | 102.103 | 34.603(0.000) | 67.500(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
DEFAULT_CLK | 100.000 | 113.238
NO CLOCK DOMAIN | 0.000 | 0.000