@N: MF284 |Setting synthesis effort to medium for the design
@N: MF916 |Option synthesis_strategy=base is enabled. 
@N: MF248 |Running in 64-bit mode.
@N: MF666 |Clock conversion enabled. (Command "set_option -fix_gated_and_generated_clocks 1" in the project file.)
@N: BN133 |Ignoring syn_hier=hard property on top-level design.
@N: MF284 |Setting synthesis effort to medium for the design
@N: MH105 |UMR3 is only supported for HAPS-80.
@N: MH105 |UMR3 is only supported for HAPS-80.
@N: MF974 |Total number of latches (multibit) processed = 0 
@N: MF975 |Total number of latches (bit blasted) processed = 0 
@N: MF976 |Total number of (multibit) opaque latches found = 0 
@N: MF977 |Total number of (bit blasted) opaque latches found = 0 
@N: FX1143 |Skipping assigning INTERNAL_VREF to iobanks, because the table of mapping from pin to iobank is not initialized.
@N: BN225 |Writing default property annotation file /home/wenbo/Desktop/Gowin_XCORR_RefDesign/XCORR_512-3_case/project/impl/temp/gao/ao_control/rev_1/ao_control.sap.
