@P:  Worst Slack : -1.318
@P:  _~DPHY_RX_DPHY_RX_TOP_|HS_CLK_inferred_clock - Estimated Frequency : 279.8 MHz
@P:  _~DPHY_RX_DPHY_RX_TOP_|HS_CLK_inferred_clock - Requested Frequency : 329.2 MHz
@P:  _~DPHY_RX_DPHY_RX_TOP_|HS_CLK_inferred_clock - Estimated Period : 3.574
@P:  _~DPHY_RX_DPHY_RX_TOP_|HS_CLK_inferred_clock - Requested Period : 3.038
@P:  _~DPHY_RX_DPHY_RX_TOP_|HS_CLK_inferred_clock - Slack : -0.536
@P:  _~idesx8_DPHY_RX_TOP_|sclk_inferred_clock - Estimated Frequency : 113.8 MHz
@P:  _~idesx8_DPHY_RX_TOP_|sclk_inferred_clock - Requested Frequency : 133.9 MHz
@P:  _~idesx8_DPHY_RX_TOP_|sclk_inferred_clock - Estimated Period : 8.786
@P:  _~idesx8_DPHY_RX_TOP_|sclk_inferred_clock - Requested Period : 7.468
@P:  _~idesx8_DPHY_RX_TOP_|sclk_inferred_clock - Slack : -1.318
@P:  System - Estimated Frequency : 244.9 MHz
@P:  System - Requested Frequency : 288.1 MHz
@P:  System - Estimated Period : 4.083
@P:  System - Requested Period : 3.471
@P:  System - Slack : -0.612
@P: DPHY_RX_TOP Part : gw1n_9pbga256-6
@P: DPHY_RX_TOP I/O primitives : 5
@P: DPHY_RX_TOP I/O Register bits : 0
@P: DPHY_RX_TOP Register bits (Non I/O) : 942 (14%)
@P: DPHY_RX_TOP Total Luts : 1010 of 800 (11%)
@P:  CPU Time : 0h:00m:09s
