@P:  Worst Slack : -0.153
@P:  _~oserx8_DPHY_TX_TOP_|sclk_inferred_clock - Estimated Frequency : NA
@P:  _~oserx8_DPHY_TX_TOP_|sclk_inferred_clock - Requested Frequency : 563.4 MHz
@P:  _~oserx8_DPHY_TX_TOP_|sclk_inferred_clock - Estimated Period : NA
@P:  _~oserx8_DPHY_TX_TOP_|sclk_inferred_clock - Requested Period : 1.775
@P:  _~oserx8_DPHY_TX_TOP_|sclk_inferred_clock - Slack : NA
@P:  System - Estimated Frequency : 979.4 MHz
@P:  System - Requested Frequency : 1152.2 MHz
@P:  System - Estimated Period : 1.021
@P:  System - Requested Period : 0.868
@P:  System - Slack : -0.153
@P: DPHY_TX_TOP Part : gw1n_9pbga256-6
@P: DPHY_TX_TOP I/O primitives : 5
@P: DPHY_TX_TOP I/O Register bits : 0
@P: DPHY_TX_TOP Register bits (Non I/O) : 0 (0%)
@P: DPHY_TX_TOP Total Luts : 0 of 800 (0%)
@P:  CPU Time : 0h:00m:04s
