Timing Analysis Report

# Timing Messages

Report Title | Gowin Timing Analysis Report
Design File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH96K_REG_IF\project\impl\synthesize\rev_1\FLASH96K_REG_IF.vm
Physical Constraints File | C:\Users\qinfei\Desktop\Gowin_Flash_Controller\FLASH96K_REG_IF\project\src\FLASH96K_REF_IF.cst
Timing Constraint File | ---
GOWIN version | V1.9.2.01Beta
Part Number | GW1N-LV1LQ144C6/I5
Created Time | Tue Oct 22 17:05:34 2019
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Timing Summaries

## STA Tool Run Summary:

Setup Delay Model | Slow 1.14V 85C
Hold Delay Model | Fast 1.26V 0C
Numbers of Paths Analyzed | 212
Numbers of Endpoints Analyzed | 598
Numbers of Falling Endpoints | 0
Numbers of Setup Violated Endpoints | 0
Numbers of Hold Violated Endpoints | 0

## Clock Summary:

Clock Name | Type | Period | Frequency(MHz) | Rise | Fall | Source | Master | Objects
--- | --- | --- | --- | --- | --- | --- | --- | ---
u_pll_10M/pll_inst/CLKIN.default_clk | Base | 20.000 | 50.000 | 0.000 | 10.000 |  |  |
u_pll_10M/pll_inst/CLKOUT.default_gen_clk | Generated | 100.000 | 10.000 | 0.000 | 50.000 |  | u_pll_10M/pll_inst/CLKIN.default_clk |
u_pll_10M/pll_inst/CLKOUTP.default_gen_clk | Generated | 100.000 | 10.000 | 25.000 | 75.000 |  | u_pll_10M/pll_inst/CLKIN.default_clk |
u_pll_10M/pll_inst/CLKOUTD.default_gen_clk | Generated | 200.000 | 5.000 | 0.000 | 100.000 |  | u_pll_10M/pll_inst/CLKIN.default_clk |
u_pll_10M/pll_inst/CLKOUTD3.default_gen_clk | Generated | 300.000 | 3.333 | 0.000 | 150.000 |  | u_pll_10M/pll_inst/CLKIN.default_clk |

## Max Frequency Summary:

NO. | Clock Name | Fmax | Entity
--- | --- | --- | ---

#### No timing paths to get frequency of u_pll_10M/pll_inst/CLKIN.default_clk!

#### No timing paths to get frequency of u_pll_10M/pll_inst/CLKOUT.default_gen_clk!

#### No timing paths to get frequency of u_pll_10M/pll_inst/CLKOUTP.default_gen_clk!

#### No timing paths to get frequency of u_pll_10M/pll_inst/CLKOUTD.default_gen_clk!

#### No timing paths to get frequency of u_pll_10M/pll_inst/CLKOUTD3.default_gen_clk!

## Total Negative Slack Summary:

Clock Name | Analysis Type | Endpoints TNS | Number of Endpoints
--- | --- | --- | ---
u_pll_10M/pll_inst/CLKIN.default_clk | Setup | 0.000 | 0
u_pll_10M/pll_inst/CLKIN.default_clk | Hold | 0.000 | 0
u_pll_10M/pll_inst/CLKOUT.default_gen_clk | Setup | 0.000 | 0
u_pll_10M/pll_inst/CLKOUT.default_gen_clk | Hold | 0.000 | 0
u_pll_10M/pll_inst/CLKOUTP.default_gen_clk | Setup | 0.000 | 0
u_pll_10M/pll_inst/CLKOUTP.default_gen_clk | Hold | 0.000 | 0
u_pll_10M/pll_inst/CLKOUTD.default_gen_clk | Setup | 0.000 | 0
u_pll_10M/pll_inst/CLKOUTD.default_gen_clk | Hold | 0.000 | 0
u_pll_10M/pll_inst/CLKOUTD3.default_gen_clk | Setup | 0.000 | 0
u_pll_10M/pll_inst/CLKOUTD3.default_gen_clk | Hold | 0.000 | 0

# Timing Details

## Path Slacks Table:

### Setup Paths Table

#### Report Command:report_timing -setup -max_paths 25 -max_common_paths 1

#### Nothing to report!

### Hold Paths Table

#### Report Command:report_timing -hold -max_paths 25 -max_common_paths 1

#### Nothing to report!

### Recovery Paths Table

#### Report Command:report_timing -recovery -max_paths 25 -max_common_paths 1

#### Nothing to report!

### Removal Paths Table

#### Report Command:report_timing -removal -max_paths 25 -max_common_paths 1

#### Nothing to report!

## Minimum Pulse Width Table:

Number | Slack | Actual Width | Required Width | Type | Clock | Objects
--- | --- | --- | --- | --- | --- | ---

#### Report Command:report_min_pulse_width -nworst 10 -detail

#### Nothing to report!

## Timing Report By Analysis Type:

### Setup Analysis Report

#### Report Command:report_timing -setup -max_paths 25 -max_common_paths 1

#### No setup paths to report!

### Hold Analysis Report

#### Report Command:report_timing -hold -max_paths 25 -max_common_paths 1

#### No hold paths to report!

### Recovery Analysis Report

#### Report Command:report_timing -recovery -max_paths 25 -max_common_paths 1

#### No recovery paths to report!

### Removal Analysis Report

#### Report Command:report_timing -removal -max_paths 25 -max_common_paths 1

#### No removal paths to report!

## Minimum Pulse Width Report:

#### Report Command:report_min_pulse_width -nworst 10 -detail

#### Nothing to report!

## High Fanout Nets Report:

#### Report Command:report_high_fanout_nets -max_nets 10

FANOUT | NET NAME | WORST SLACK | MAX DELAY
--- | --- | --- | ---

## Route Congestions Report:

#### Report Command:report_route_congestion -max_grids 10

GRID LOC | ROUTE CONGESTIONS
--- | ---
R7C9 | 0.500
R4C8 | 0.472
R1C20 | 0.458
R4C5 | 0.431
R4C6 | 0.403
R7C10 | 0.375
R5C12 | 0.375
R4C7 | 0.375
R4C4 | 0.361
R7C12 | 0.347

## Timing Exceptions Report:

### Setup Analysis Report

#### Report Command:report_exceptions -setup -max_paths 5 -max_common_paths 1

#### No timing exceptions to report!

### Hold Analysis Report

#### Report Command:report_exceptions -hold -max_paths 5 -max_common_paths 1

#### No timing exceptions to report!

### Recovery Analysis Report

#### Report Command:report_exceptions -recovery -max_paths 5 -max_common_paths 1

#### No timing exceptions to report!

### Removal Analysis Report

#### Report Command:report_exceptions -removal -max_paths 5 -max_common_paths 1

#### No timing exceptions to report!

## Timing Constraints Report:

SDC Command Type | State | Detail Command
--- | --- | ---