Power Analysis Report

- Power Messages
- Power Summary
  - Power Information
  - Thermal Information
  - Configure Information
  - Supply Information
- Power Details
  - Power By Block Type
  - Power By Hierarchy
  - Power By Clock Domain

# Power Messages

Report Title | Gowin Power Analysis Report
Design File | E:\GOWIN_WORK\IP_Design\MIPI\MIPI_release_case\MIPI_DPHY_Reference_Design\MIPI_RefDesign\impl\synthesize\rev_1\MIPI_RefDesign.vm
Physical Constraints File | E:\GOWIN_WORK\IP_Design\MIPI\MIPI_release_case\MIPI_DPHY_Reference_Design\MIPI_RefDesign\src\mipi.cst
Timing Constraints File | E:\GOWIN_WORK\IP_Design\MIPI\MIPI_release_case\MIPI_DPHY_Reference_Design\MIPI_RefDesign\src\mipi.sdc
GOWIN Version | V1.9.3Beta
Part Number | GW1N-LV9PG256C5/I4
Created Time | Mon Mar 30 11:17:39 2020
Legal Announcement | Copyright (C)2014-2019 Gowin Semiconductor Corporation. All rights reserved.

# Power Summary

## Power Information:

Total Power (mW) | 51.152
Quiescent Power (mW) | 3.690
Dynamic Power (mW) | 47.462

## Thermal Information:

Junction Temperature | 25.520
Theta JA | 10.200
Max Allowed Ambient Temperature | 84.478

## Configure Information:

Default IO Toggle Rate | 0.125
Default Remain Toggle Rate | 0.125
Use Vectorless Estimation | false
Filter Glitches | false
Related Vcd File |
Related Saif File |
Use Custom Theta JA | false
Air Flow | LFM_0
Heat Sink | None
Use Custom Theta SA | false
Board Thermal Model | None
Use Custom Theta JB | false
Ambient Temperature | 25.000

## Supply Information:

Voltage Source | Voltage | Dynamic Current(mA) | Quiescent Current(mA) | Power(mW)
--- | --- | --- | --- | ---
VCC | 1.200 | 38.411 | 2.345 | 48.907
VCCX | 2.500 | 0.250 | 0.156 | 1.016
VCCO12 | 1.200 | 0.009 | 0.003 | 0.014
VCCO25 | 2.500 | 0.069 | 0.042 | 0.277
VCCO33 | 3.300 | 0.169 | 0.115 | 0.937

# Power Details

## Power By Block Type:

Block Type | Total Power(mW) | Static Power(mW) | Average Toggle Rate(millions of transitions/sec)
--- | --- | --- | ---
Logic | 4.539 | NA | 12.500
IO | 2.729 | 1.065 | 14.258
BSRAM | 0.749 | NA | NA
PLL | 0.785 | NA | NA

## Power By Hierarchy:

Hierarchy Entity | Total Power(mW) | Block Dynamic Power(mW) | Routing Dynamic Power(mW)
--- | --- | --- | ---
DPHY_TOP | 45.397 | 5.698(5.529) | 39.699(38.112)
DPHY_TOP/u_DPHY_RX_TOP/ | 41.559 | 4.154(4.154) | 37.405(37.405)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/ | 41.559 | 4.154(4.154) | 37.405(37.345)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/ | 40.304 | 4.146(4.144) | 36.157(36.145)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk1.wd3/ | 8.175 | 0.759(0.000) | 7.416(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk2.wd2/ | 7.913 | 0.770(0.000) | 7.143(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk3.wd1/ | 7.519 | 0.767(0.000) | 6.752(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk4.wd0/ | 7.798 | 0.770(0.000) | 7.028(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk6.ln0/ | 8.884 | 1.077(0.646) | 7.806(3.669)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk6.ln0/genblk10.U1/ | 1.136 | 0.159(0.000) | 0.977(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk6.ln0/genblk11.U2/ | 1.078 | 0.167(0.000) | 0.911(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk6.ln0/genblk12.U3/ | 0.965 | 0.159(0.000) | 0.806(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_Aligner/genblk6.ln0/genblk9.U0/ | 1.137 | 0.162(0.000) | 0.975(0.000)
DPHY_TOP/u_DPHY_RX_TOP/DPHY_RX_INST/u_idesx8/ | 1.196 | 0.008(0.000) | 1.188(0.000)
DPHY_TOP/u_DPHY_TX_TOP/ | 0.836 | 0.700(0.700) | 0.136(0.136)
DPHY_TOP/u_DPHY_TX_TOP/DPHY_TX_INST/ | 0.836 | 0.700(0.700) | 0.136(0.136)
DPHY_TOP/u_DPHY_TX_TOP/DPHY_TX_INST/u_oserx8/ | 0.108 | 0.003(0.000) | 0.106(0.000)
DPHY_TOP/u_DPHY_TX_TOP/DPHY_TX_INST/u_pllx8/ | 0.727 | 0.697(0.000) | 0.030(0.000)
DPHY_TOP/u_ROM549x17/ | 1.158 | 0.588(0.000) | 0.570(0.000)
DPHY_TOP/u_plld4/ | 0.089 | 0.087(0.000) | 0.002(0.000)

## Power By Clock Domain:

Clock Domain | Clock Frequency(Mhz) | Total Dynamic Power(mW)
--- | --- | ---
clk_tx | 100.000 | 2.011
clk_rx | 100.000 | 42.596
u_plld4/pll_inst/CLKOUT.default_gen_clk | 3.125 | 0.699
u_DPHY_TX_TOP/DPHY_TX_INST/u_pllx8/pll_mipi_tx/CLKOUTP.default_gen_clk | 25.000 | 0.015
u_DPHY_TX_TOP/DPHY_TX_INST/u_pllx8/pll_mipi_tx/CLKOUT.default_gen_clk | 25.000 | 0.015
u_plld4/pll_inst/CLKIN.default_clk | 50.000 | 0.087